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External Walls


Facing brick (Light grey with matching mortar) -
Wienerberger: Terca Clay Brick

[image: A white brick wall

Description automatically generated with medium confidence]










Wooden Wall –
 Benchmark Timber : Western Red Cedar Timber
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Description automatically generated]









Dark Colour Timber Cladding – 
Harleston Supplies: Feather Edge 4.8m Black Timber Cladding

[image: A close up of a wood surface

Description automatically generated with medium confidence]







Roof

Roof – Slate Tiles
Roofing Superstore: Cwt Y Bugail County Grade Welsh Slate Roof Tile in Blue/Grey
[image: A solar panel on a roof

Description automatically generated with medium confidence]




Windows and Doors – High Performance Aluminium
Windows and Doors

Windows and Doors – High Performance Aluminium
Norrsken – Aluminium windows and door colour
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Description automatically generated with medium confidence]
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7016 Anthracite Grey
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S't SHAUN-TANNER




