Planning application No. 150721
Discharge of Condition 15 - Sound Mitigation Measures
Condition 15
Prior to first occupation of any residential unit hereby permitted, details of measures to protect future occupiers from the external noise environment shall be submitted to and approved, in writing, by the Local Planning authority. Such measures shall relate to the specifications stated in “Noise Survey and Assessment by Philip Acoustics Ltd Ref 15068-002 dated June 2015, as received 08/06/15” and Supplementary Noise Report by Philip Acoustics Ltd dated 23.12.15 Ref 15068-004, as received 19/01/16”. The approved measures shall be carried out in full and completed prior to first occupation of any residential unit permitted, and retained thereafter.
Two sound reports were submitted and referenced in the planning approval notice and are referenced above for ease of reference. Where there is a difference in recommendation between the original report and the supplementary report the higher requirements will be implimented

External walls and roof.
· Ceilings underneath both the flat roof areas and pitched roof areas to be upgraded to a  double layer of 15mm SoundBloc plasterboard with mineral wool insulation in the void
· Cavity blockwork walls with an internal plasterboard lining of 1 x 12.5mm SoundBloc plasterboard throughout.
Glazing
· Asymmetric double glazing with 6.7mm – 18mm air gap – 4mm glass to be fitted to windows
· Secondary glazing to all windows
· Neoprene beaded “P” type compresses all around.
Ventilation
· Mechanical ventilation to be fitted to each flat
· All ventilation apertures will be located on side elevations or at roof level. None will be located on the Northern elevation
· The overall self-noise from the system to be no higher than 25dB

The above specification is considerably higher used in standard construction and as a consequence of this, the implementation of the above measures will provide high protection against the higher noise levels caused by Face Bar.

