Design and access statement
Flat 5 Springfield House, 24 Surley Row, Emmer Green, RG4 8LY
Aim
To replace 4 single glazed windows and 1 single glazed French door with double glazing to reduce condensation and mould issues within the property and improve quality of life of the residents. 
[bookmark: _GoBack]All windows and doors will remain timber and cottage style but the windows will be vertical sliders to fit with fire regulations that require windows to be bottom-opening. All waste and mess will be removed by the installation company and parking for the installers is available in the forecourt. 
Current windows:
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Current French door:
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Replacement windows:
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