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Drainage strategy.


The site will be developed for an artificial pitch tennis hall and earthworks to infill the dip in the playing fields. The pitch itself will not generate surface water run off but will in fact maintain the existing situation if not improve it.  There are no gulleys or drains around the outside of the pitch to take surface water run off as it will not occur.  The tennis hall will be located onto the already impermeable hard surface of the tennis courts but will be served by a new soakway which can be placed in the most beneficial position as opposed to the current position where water runs off around the courts.
[bookmark: _GoBack]The pitch is constructed, and acts, as a large soakaway.  Rainwater percolates through the artificial grass and the sand ballast through a porous tarmac into the sub-base of a minimum 250mm of Type 1 stone.  This is separated from the base soils by a terram layer to prevent stone and soils mixing. Therefore, it will drain better than the natural soils. 
There is no evidence that flooding is an issue as a result and inspection of the excavated soil deposited materials indicate that the ground is free draining stony base and we consider no further investigations are required. 
Below the artificial grass and permeable tarmac layer is a 250mm layer of type 1 stone and then a herringbone drainage system at 10m intervals with a perimeter system beneath the pitch as a belt and braces approach to the draining of the site (see edge detail on submitted plans).  The levels on this site are consistent with those required for the Artificial pitch to leave the site with a 1:100 slope (approx). This slope is to ensure that water is not left pooling or standing on the surface for any period of time in the event of a substantial rain fall event.  It will not flow off the pitch as the carpet will control the water before draining through the porous tarmac level.  The sub base in this area is amenable to soakaways as stated above. 
The drains and soakaway will be set at 600mm depth, which is 300mm below the level of the stone in the sub base of the soils and at set at 10m intervals.  By the time that water reaches these levels it is already permeated into the soil base levels.  As a result the drains and soakaway system is rarely used and water at best will be a trickle into the soakaway.   The soakaway will be modest in size commensurate to the size of the pitch They are most effective in already wet landscapes as opposed to dealing with water generated off the surface.  
Wet soils around the drains will be assisted by the drainage system.  As this site does not fall into a flood zone liable to flood we conclude that the pitch will aid surface water percolation over the existing grass area. 
The main issue in relation to maintaining the drainage regime is to ensure that the pitch is properly looked after.  It is usual that the pitch would be maintained once a week to allow movement of the sand ballast so that it cannot become clogged with detritus.  Deep cleans are usually undertaken by the contractors company at least once a year.  Assuming that this is done, and it is in the interests of the school for performance reasons as well as drainage, there is unlikely to be any issues relating to pooling of water or reduced drainage capacity.
Overall we would expect to see an improved situation regarding drainage of soil as a result of the artificial turf development.
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