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I. The parking of vehicles of site operatives and visitors
A total of 11 spaces are proposed, a further 2 spaces are available until the disabled space and bin store are completed. These spaces can be used for parking and for storage as shown on drawing 2737 003P1. 

No Parking of site personnel, operatives, contractors and visitors will take place on the public Highway at any time. 

[bookmark: _GoBack]Contractor should note that there is a right of way across the site which is to be kept free at all times, as is the undercroft to 3-4 Wesley Gate.

Location of parking spaces and stores can be swapped between the different sides if needed by the contractor, both areas are clearly identified by hatch on 2737 003P1.



II. Location on site for storage of plant and materials used in constructing the development
Safe and secure plant and material storage areas will be utilised as the overall site 
develops. The site compound will be sub-divided into trade specific sections if possible, and will facilitate the safe segregation of materials (flammable/non- flammable, etc). 

There will be a permit system in place for the issue of keys for the plant on site, and all vehicles will be locked and secured at the end of each working day and the keys returned to the site management for safe keeping. All plant and materials will be stored on site. No Storage of plant or materials will be undertaken on the Public Highway at any time.

All waste material generated from the conversion and new build will be stored in the designated secured skip. See drawing 2737 003P1. 



III. The erection and maintenance of security hoarding where appropriate
The site will be surrounded by the appropriate hoarding to ensure that it is kept secure. Where timber hoarding is used it will be painted and will display all the appropriate signage.  

Barriers on or abutting the highway will comply with Chapter 8 of the Dept. Transport Traffic Signs Manual. All hoarding and scaffolding will be kept within the confines of the site and as such a scaffolding/hoarding licence should not be required. If necessity arises for hoarding to be constructed on public highway, the contractor must apply for a licence. See drawing 2737 003P1. 

Barriers are not assumed to impact on Wesley Gate 



IV. Any footpath closures or road closures needed during construction
There is no need to close any road or footpath for construction



V. Wheel washing facilities
Wheel washing facilities will be provided at the entrance to ensure there is no transfer of mud and debris to the road. See drawing 2737 003P1. 



VI. A scheme for recycling waste resulting from the construction programme
A scheme will be implemented with the contractor’s waste collection sub-contractor to sort all waste into to different piles and these will be recycled where possible. All skips collected from site are subject to sorting at their recycling station. 


VII. Provisions to be made for the control of noise and dust coming from the site during demolition and construction
Nuisance from dust created from the works will be minimised through pre-fabrication off-site. Where this is not possible operations will be carried out in a designated area using dust extraction and filters on the cutting tools. Regular damping down and the use of suitable screens to prevent dust spreading will keep dust creation during demolition etc. to a minimum.  Dust will be regularly cleared up using suitable vacuum devices. Sweeping, which tends to spread dust, will be avoided where possible. Any land clearing activities will be “damped down” using water suppression. Loaded lorries and skips will be covered with netting/sheeting, and the wheels of vehicles/plant leaving site will be cleaned when required so that dirt is not spread onto the surrounding roads.


VIII. Arboricultural report

There are important arboricultural requirements on site: please refer to the method statement and tree protection plan prepared by GHA arboriculturalist. 

If in doubt please contact Glen Harding the arboriculturalist on 07884 056025


IX.             Hours of working

The permitted hours are:

· Monday to Saturday: 8.00am to 6.00pm 
· Sundays and Bank Holidays: No Noisy Work

All site deliveries to site currently are scheduled within the early morning generally, and this has not caused any issues.  The contractor is advised to continue site deliveries as currently taking place for the PD element of the scheme. 
The contractor should consider avoiding congestion at peak times if this situation changes.

All site personnel will be given a Site Induction by the Site Agent in which they will be informed of all matters in the Method Statement, including those regarding parking and unloading. 
 
Immediate neighbours affected by the works will be advised of timing and progress of the works and will be provided with contact names and telephone numbers for site management who will deal with any queries or concerns. 

It should be noted that existing works as part of the PD development have not caused any issues, and the contractor has maintained good contact with neighbours. 
In exceptional circumstances (for example, in the case of police traffic restrictions or in an emergency) work outside these hours may be unavoidable. In such cases the person responsible will advise adjoining occupiers prior to work taking place.
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