Front elevation windows – 

Run-through Horn - Standard
Meeting Stile - 35mm
Corner Detail - Mechanical
Woodgrain - Standard
Deep Bottom Rail - Standard
85mm Slim Mullion
Locks - Globe Hook
Profile Detail - Putty Line
Rear elevation new windows - 
· Soft coat Low E 24mm Argon filled double glazed units providing excellent thermal efficiency with a u value of 1.4 W/m² K. Complies with the A rating as used by the British Fenestration Rating Council.
· Eco friendly plastic thermal reinforcement
· Strong hardwearing 70mm multi chamber PVCu frame that is virtually maintenance free and won't flake, rot, peel or rust.
· Secure locking system. Internally beaded for added security
· Complies with Building Regulations Part L and Part F and Scottish Section 7
· No need to deglaze when installing with fixing cleats
· Trickle vent system allowing clean fresh air ventilation even when the window is locked and secure.
· UK manufactured with 10 year manufacturer guarantee, Sill and handles are not included
· Sizes shown are actual window sizes. Add 30 mm to the height for the sill and 10mm for opening brick work dimensions
· Recommended Cavity Closers for this window are for a 100mm cavity SKU 176384 and for a 125mm cavity SKU 176401
Smoke vent – 
· 10 year guarantee on windows and flashings.
· 3 year guarantee on all electrical products and accessories.
· 4mm toughened outer pane with low-E coating.
· Offers improved noise reduction compared to - -34 and - -59 glazing.
· 6.4mm laminated inner pane offers additional safety.
· 114cmx 118cm.
Natural slate – 
Sizes: 500x250mm, 400x250mm
Grades: Prime – 7mm Nominal Thickness
Testing: BSEN12326-1:2004 – A1, T1 & S1






Skylights – 

Manually operated, high quality VELUX roof window with a stylish white frame. Roof window’s features include: 

· Premium quality roof window.
· Manually top-operated centre-pivot roof window is easy to operate, even with furniture beneath. VELUX white painted roof window gives your home a bright and sophisticated look.
· White painted roof windows are painted then coated with a water-based lacquer, sealing and protecting the wood from dirt and moisture. The bright white finish works with all modern interiors and is low maintenance, staying beautiful longer than an unpainted window.
· Classic frame design with great strength and precise contours.
· ThermoTechnology™ boosts your home's comfort and helps decrease the energy bills. It places high-performance energy-efficient materials directly into the window construction, increasing the insulating properties of the window and creating an airtight seal.
· Equipped with a filter blocking dust and insects.
· Ventilation flap lets you enjoy clean, fresh air without having to open your window. This allows fresh air to enter but maintains security and keeps rain and wind out.
· 4 glazing options: double glazed, triple glazed panes with many features available. Choose a glazing that fits your needs best – and you can save energy, reduce noise or improve safety.
· This white painted roof window is suitable for roof pitches between 15 - 90 degrees.
· 180 degrees rotation - for easy cleaning of the external pane and with locks in position feature.
· Easy to maintain.
· 10 years guarantee.
· 550x780mm

Wickes Upvc French Doors With 2 Side Panels– 

2090x 2390mm
Opening Direction: Outwards
Glazing Type: Clear Double Glazed
Includes: Frame & Hardware
Heat Loss U Value: 1.8 W/m2K
Years Guaranteed: 10
Standards Met: BS EN 1279. Part L
Brand Name: Wickes


Universal black fascia board 

	Width (Imperial)
	9"

	Width
	225mm

	Length
	5m

	Thickness
	10mm

	Finish
	Black

	Material
	PVCu

	Use
	Internal / External use


Once Weathered Coping – With Drip Grooves
	Overall Size (Width x Length)
	Height (max)
	Height (min)
	Weight
	Drip Grooves
	Product Code

	 400mm x 600mm
	 75mm
	 50mm
	 34.5kg
	 Yes
	 OW-400



FLoPlast Square Line Gutter header - 
Depth: 137 mm
Height: 142 mm
Width: 142 mm
Material: PVCu
Colour: Black
Pack Quantity: 1
Years Guaranteed: 10

FloPlast RPS2.5B Square Line Downpipe - Black 65mm x 2.5m – 

Depth: 68 mm
Length: 2500 mm
Width: 68 mm
Material: PVCu
Colour: Black
Pack Quantity: 1
Years Guaranteed: 20

Composite Basement Front door – 
● Solidor composite doors are PAS23-24 compliant.
● The ultimate composite door for security and durability.
● All Glass used at Solidor Composite Doors is Toughened to British Standards.
● All sealed units used in Solidor Composite Doors are compliant with BSEN1279.
● Solidor hold BSI ISO 9001 and Secured by design accreditation.


Hampshire stock red multi ATR – 

Gross Dry Density: 1400 kg/m3
Compressive Strength: 6 N/mm2
Water Absorption: 18%
Thermal Conductivity: 0.41 W/m.K-50% - 0.47 W/m.K-90%
Dimensions: 215mm x 102.5mm x 65mm

Slip Cill – 

[image: ]
Stair railing – 

Wall Fix Handrail
Our wall fix handrails are made to order using 40mm x 12mm D shaped bar and come with decorative fixing brackets measuring 200mm high x 105mm wide x 90mm deep.  The elegant scrolled ends are 120mm wide.
They can be fitted at any angle with the brackets supplied.  The maximum projection of the handrail is 110mm measured from the wall to the outside edge of the scroll.
Gate and railing – 
Made to order using 12mm solid square vertical steel bars spaced at 100mm intervals (4″), framework is 30mm x 8mm (1.18″ x 0.31″) flat bar horizontal bars and 30mm (1.18″) SHS (square hollow section) verticals.
The ball top railheads are 100mm x 25mm on a 12mm square base.  Also included free of charge is a fixing kit comprising brackets, hinges, latches, nuts and bolts.
Why not upgrade to 16mm solid vertical bars? Contact us for a quote.
[bookmark: _GoBack]Please note that we make the 914mm (3ft) and 1220mm (4ft) high gates with one row of decoration and the 1830mm (6ft) high metal gates with two rows of decoration.
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