MORNINGWOOD LTD

NEW DWELLING, 92 LOWER HENLEY ROAD, CAVERSHAM, READING, RG4 5LE
RISK ASSESSMENTS

	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	SITE CABIN OFFICES etc

Placing and Removal


	Site activity and condition

Ground conditions

Overhead Services

Existing structures

Falls of cabins

Inclement weather - high winds

Other persons incl public

Lorry Manoeuvres

Head, Eye, Hand and Foot Injury
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR THE PLACING AND REMOVAL OF SITE CABINS ETC.

Works to be carried out by experienced and competent persons, briefed as to Method Statement/Risk Assessment.

Overhead services to be protected, goalposts etc, isolated prior to work commencing.

Firm ground for lifting equipment with adequate space for outriggers and delivery lorries.

Lifting equipment (SWL) to safely lift all cabins etc in good order, certificated, weekly inspections to be confirmed on standard report form.

Operated by certificated (CITB) driver and assisted by certificated (CITB) banksman/slinger wearing Hi-Vi vest.

Tail rope to be used to guide cabins.

SAFETY HELMETS & FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, Hi-Vi vests to be used as per RISK/COSHH Assessments.

Lorries to observe speed limits and assisted by banksman wearing Hi-Vi vest during reversing manoeuvres.

Work to cease during inclement weather - high winds.

Work area to be barricaded to protect other persons.


	Contract Manager to provide

Site Manager

Site Manager




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	UNAUTHORISED ACCESS ONTO SITE
	Site working conditions and operations of work

Storage areas

Site transport

Plant and equipment

Personal injury

Theft and unauthorised use of site transport, plant and equipment

Damage to site transport, plant, equipment and materials
	Notices posted to instruct all visitors to report to the Site Manager's office.

A 2m high Heras Fence/Hoarding will be positioned around the site boundary with secured gates provided at access points.

Additional fencing etc. will be provided and positioned to deter children entering site.

Notices will be posted at access and intermediate points warning of the hazards of construction work.

All offices, storage containers, site transport etc. will be made secure when not in use.

All plant and equipment will be isolated and stored securely when not in use.

All ladders will be removed to secure storage or made inclimbable at the end of the working day.

All manholes will be securely covered.

All open excavations will be either securely fenced or covered at the end of the working day.

Safety talk will be given to children while working in or adjacent to schools.


	Site Manager

Safety Manager




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	DEMOLISHING
	Site activity and conditions

Falls of material, debris and persons

Head, eye, hand and foot injury

Dust and splashes

Noise

Personal Hygiene

Nails in Timber

Collapse of Structure

M/C operations

Lorry Manoeuvres

Drug abuse equipment

Contaminated waste

Existing services - gas, water

and electricity (underground/overhad)

Other persons incl public 

Fire

Electrocution

Access and Egress
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR DEMOLISHING WORK, INCLUDING ALL TEMPORARY WORKS PROVISION NECESSARY TO ENSURE A SAFE SYSTEM OF WORK.

Work to be carried out by experienced and competent persons, briefed as to Method Statement/Risk Assessment.

Existing services located, marked and isolated prior to work commencing.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, respiratory protection, harnesses, overalls and hearing defenders used as required - COSHH/RISK/NOISE ASSESSMENT.

Personal hygiene maintained, all cuts and abrasions covered.  Tetanus reminder to all operatives.

Ground to be firm for stability of M/C's lorries, scaffolding etc.

Fully boarded bandstands, scaffolds, level with guard-rails, toeboards and mesh if over 2m high (all scaffold to be secured in position).  Debris netting, fans erected to protect other persons inc public, weekly inspections recorded on standard report forms.

Waste to be bagged and chuted/lowered to ground.

All timber de-nailed - no throwing (bombing).

All plant and equipment to be in good order and covered by a current test certificate (weekly inspections recorded on standard report forms) and operated by Certificated (CITB) persons. Electrical tools 110 volts only.

Banksman to assist reversing lorries (Hi-Vi vest worn)

Fire extinguishers positioned in all work areas.

NO BONFIRES ON SITE
	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	DEMOLISHING CONTINUED
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Local Authority to advise on disposal of drug abuse equipment etc.

A copy of waste transfer noted required.

A safe means of access and egress to all work areas maintained.

Warning signs of overhead work, in position
	Contractor

Site Manager




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	ASBESTOS REMOVAL

- Pipe Lagging

- Sheet

- Waste
	Site activity and conditions

Asbestos fibres

Personal Hygiene

Asbestos waste

Other persons inc public 

Fire

Electrocution

Access and Egress

Head and Foot Injury

Existing services - Gas, water & electricity

Falls of persons
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR ALL ASBESTOS REMOVAL

LICENSED ASBESTOS REMOVAL CONTRACTOR TO UNDERTAKE WORK WHERE NECESSARY
Work to be carried out by experienced and competent persons, briefed as to Method Statement/Risk Assessment.

Existing services located, marked, protected, isolated prior to work commencing.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

All other PPE to be used in accordance with method statement/Risk Assessment.

Personal hygiene standards maintained.

Work area screened to prevent spread of fibres and warning notices erected.

A copy of waste transfer note required.

A copy of all air monitoring results required.

No hotwork allowed in tended area.

Electrical tools 110 volts only and covered by current test certificate.

All waste to be classified as 'Asbestos contaminated and transferred from site double bagged and listed as 'Asbestos Waste'.

All access equipment to be firm, level, fully boarded with guardrails, toeboards and mesh in position if over 2M high (scaffold inspections recorded weekly standard report forms.  Stepladders in good order.

All access equipment to be thoroughly decontaminated before removal from site.


	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	EXCAVATION AND EARTHWORKS

- Underpinning

- Foundations

- Removal of Oversite

- Drainage
	Site activity and conditions 

Collapse of excavations

Falls of materials and persons

Access and egress

Contaminated ground

Head, eye, hand and foot injury

Dust and splashes

Noise

Manual handling injury

M/C operations

Site transport & lorry manoeuvres

Existing services - gas, water and electricity (underground/overhead)

Adjacent/sources of water - flooding 

Electrocution

Personal Hygiene

Mud on  Access Roads

Other persons incl public
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR ANY EXCAVATION WORK DEEPER THAN 1.2M AND FOR ALL WORK IN CONTAMINATED GROUND

Work to be carried out by experienced and competent persons, briefed as to Method Statement/Risk Assessment.

Survey site, locate, mark, protect, isolate services prior to work commencing.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, respiratory protection, Hi-Vi vests, overalls, wet weather clothing and hearing defenders as required - RISK/COSHH/NOISE ASSESSMENT

Personal hygiene maintained, all cuts and abrasions covered, tetanus and weils disease reminders to operatives.

Ground to be firm for stability of M/Cs. lorries etc.

A safe means of access and egress for operatives and site transport, maintained, warning signs posted.

All site transport/lorries to observe speed limit and assisted by banksman when reversing.

Excavations/earthworks adequately supported to prevent collapse, daily inspection (weekly inspections recorded on standard report form).

Secured means of access and egress provided into and across excavations.

Physical barriers erected to prevent falls of persons, materials and M/Cs into excavations

Warning signs positioned.


	Contract Manager to obtain from contractor

Contractor




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	EXCAVATION AND EARTHWORKS Continued
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All plant and equipment to be in good order and covered by a current test certificate and operated by certificated (CITB) persons

Electrical tools 110 volts only

Access road to be kept clean

A copy of waste transfer note required

MANUAL HANDLING/JOB SPECIFIC RISK ASSESSMENT to determine method of lifting materials etc

Pumps provided to prevent flooding, check with local NRA office on discharge restrictions and permission.
	Site Manager

Site Manager




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	PILING

- Auger

- Driver

- Vibration
	Site activity and conditions

Ground conditions

Contaminated Ground

Existing Services - underground and overhead

Access and Egress

Head, eye, hand and foot injury

Splashes, personal hygiene

Noise

M/C operations

Site transport and lorry manoeuvres

Other persons incl public

Mud on access roads

Protruding bars from pile caps

Inclement weather - high winds
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR ALL PILING OPERATIONS OF WORK

Work to be carried out by experienced and competent persons, briefed as to Method Statement/Risk Assessment.

Survey site, locate, mark, protect, isolate services prior to work commencing.

Ground to be firm for piling rig stability, M/Cs & lorries etc

Safe means of access and egress maintained for operatives and site transport etc warning signs positioned 

All site transport/lorries to observe speed limit and assisted by banksman when reversing.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME - Gloves, eye protection, respiratory protection, harnesses, Hi-Vi vests, overalls, wet weather clothing and hearing defenders used as required - RISK/COSHH/NOISE ASSESSMENT

Site transport/piling rigs to be in good order certificated (weekly inspections recorded on standard report form) and operated by certificated (CITB) persons

Access roads to be kept clean

All vehicles leaving site to have wheels washed 

A copy of waste transfer note required

MANUAL HANDLING/JOB SPECIFIC RISK ASSESSMENT to determine method of lifting materials etc.

Protruding bars to be covered/fenced to prevent persons falling onto them

Warning signs erected ref 'operations at work' 

Work to cease during inclement weather
	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	TOWER CRANE

- Erection and Dismantling
	Site activity and conditions

Ground conditions

Overhead and underground services

Existing structures

Access and egress

Falls of persons and materials

Inclement weather - high winds

Other persons incl public

Lorry manoeuvres

Head, eye, hand and foot injury
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR THE ERECTION AND DISMANTLING OF A TOWER CRANE

Work to be carried out by experienced and competent persons, brief as to Method Statement/Risk Assessment.

Overhead services to be protected, goalposts, warning signs etc.  Underground services to be located, marked, protected, isolated prior to work commencing.

Firm ground for mobile crane stability, adequate space for crane outriggers and delivery lorries etc

Mobile crane (SWL) to safely lift all tower crane competent parts, in good order, certificated, weekly inspection on standard report form and operated by certificated (CITB) driver and assisted by certificated (CITB) banksman slinger wearing Hi-Vi- vest.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, harness, Hi-Vi vest to be used on required RISK/COSHH Assessment Work to cease during inclement weather, eg, high winds

Work to be barricaded, with warning signs erected.

Banksman to assist reversing lorries.

Tail ropes to guide sections into position.


	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	ERECTION OF STRUCTURES

- Steel Frame

- Concrete Beam
	Site activity and conditions

Ground conditions

Overhead services

Access and Egress

Head, eye, hand and foot injury

Falls of persons and materials

Plant and M/C operations

Other persons incl public

Site transport and lorry manoeuvres

Collapse of structure

Inclement weather - high winds
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR STEEL ERECTION

Work to be carried out by competent persons, briefed as to Method Statement/Risk Assessment.

Overhead services to be protected - goalposts etc/isolated, prior to work commencing.

Firm ground for mobile crane stability.

Adequate space for crane outriggers and access equipment etc.

Mobile crane lifting capacity to safely lift all beams, in good order, certificated.

Weekly inspections recorded on standard report form operated by certificated (CITB) driver and assisted by certificated (CITB) banksman wearing Hi-Vi vest.

Access for bolting operations by means of secured ladders access or powered platform - NO BEAM WALKING  - SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME.

Gloves, eye protection, harnesses and Hi-Vi vest used as required.  RISK/COSHH ASSESSMENT

All slinging to be carried out by certificated (CITB) person.

No throwing of bolts, tools etc, to be hoisted/lowered.

Structure to be braced to prevent collapse.

Site transport and lorries to observe speed limits, fitted with reverse alarms and assisted by a banksman.

Work area to be barricaded and warning signs erected.

Work to cease during inclement weather (high winds)

Beam release system to be used.

Tail ropes to guide beams into position


	Contract Manager to obtain from contractor

Contractor

Site Manager




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	FORMWORK


	Site activity and conditions

Falls of persons and materials

Access and Egress

Collapse of formwork

Manual handling injury

Head, eye, hand and foot injury

Dust and splashes

Noise

Plant and M/C operations

Other person, incl public

Housekeeping

Electrocution

Inclement weather - high winds in exposed elevations

Nails in timber

Striking


	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR ALL FORMWORK OPERATIONS OF WORK WHICH MUST INCLUDE CALCULATIONS AND THE DESIGN SUPPORT SYSTEMS TO PREVENT COLLAPSE

Work to be carried out by experienced and competent persons, briefed as to requirements of the Method Statement/Risk Assessment.

Fully boarded bandstands, scaffold towers, scaffold with guardrails, toeboards and mesh in position if over 2M high.  Fans and debris netting positioned to protect other persons, public etc.

All ladders providing access and egress to be secure.

Guardrails, toe boards and mesh/debris netting to be positioned to prevent falls of persons from decking if over 2M high.

Design support system to be checked prior to concrete pour.

SAFETY HELMETS & FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, respiratory protection harnesses, Hi-Vi vests and hearing defenders used as required - RISK/COSHH/NOISE ASSESSMENT MANUAL HANDLING/JOB SPECIFIC RISK ASSESSMENT TO DETERMINE METHOD OF LIFTING MATERIALS ETC

Plant & equipment to be good order, guarded etc.

All electrical tools 110 volts only and covered by a current test certificate.

Work area to be kept clean and tidy, waste removed daily.


	Contract Manager to obtain from Contractor

Contractor


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	FORMWORK

Continued
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All timber de-nailed

Warning signs erected to warn of overhead work

Work to cease during inclement weather (exposed, high elevations)

Certified (CITB) banksman to assist lifting operation

All waste to be lowered to the ground. 

No throwing (bombing) allowed.

Tail ropes to be used to guide wood panels into position etc
	Site Manager

Contractor

Site Manager




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	SCAFFOLDING

- Erection

- Adaption

- Dismantling
	Site activity and conditions

Ground conditions

Overhead services

Existing structures

Access and egress

Falls of persons and materials

Other persons incl public

Head, foot, eye and hand injury

Manual handling

M/C accidents

Lorry manoeuvres

Collapse of scaffold

Inclement weather, eg high winds
	METHOD STATEMENT/JOPB SPECIFIC RISK ASSESSMENT FOR THE ERECTION, ADAPTION AND DISMANTLING OF SCAFFOLDING

Work to be carried out by experienced and competent persons CITB certificated, briefed as to METHOD STATEMENT/RISK ASSESSMENT.

Overhead services isolated or protected with goalposts signs erected to warn of position.

Ground conditions to be firm level and clear of site debris etc for basing out scaffold.

SAFETY HELMETS & FOOTWEAR TO BE WORN ALL TIME.

Gloves, eye protection, harnesses to be used as per RISK ASSESSMENT.

MANUAL HANDLING ASSESSMENT TO DETERMINE METHOD OF LIFTING SCAFFOLD EQUIPMENT.

Lifting equipment to have current test certificate 

Weekly inspections recorded on standard report form.

Scaffold to be braced/tied/strutted to prevent collapse.

Work to cease during inclement weather eg high winds

NO THROWING OF SCAFFOLD CLIPS, TUBES ETC

Work to be barricaded to protect other fans erected persons and public, signs erected warning of work in progress.

INCOMPLETE SCAFFOLD SIGNS TO BE ERECTED FOR UNFINISHED/INCOMPLETE SCAFFOLDING

Ladders providing access correct length, good condition and secured.

Lorries to observe speed limits and assisted by a banksman in Hi-Vi vest during reversing manoeuvres.


	Contract Manager to obtain from Contractor

Contractor

Site Manager




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	SCAFFOLDING

Continued
	
	All tube ends and clips to be protected.

HANDING OVER CERTIFICATE REQUIRED FOR ALL ERECTION AND ADAPTION SCAFFOLD WORK

All lifts above 1.8M to be fitted with guardrails and toeboards.

Scaffolders to wear harnesses on lifts above 1.8M to prevent falls of persons.

Alternate scaffold tube lengths to avoid "hinging"


	Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	PRE-CAST CONCRETE FLOOR INSTALLATION

- Pot and Beam Slab


	Site activity and conditions

Ground conditions

Overhead services

Existing structures

Access and Egress

Head, eye, hand and foot injury

Falls of persons and materials

Plant and M/C operations

Other persons incl public

Lorry manoeuvres

Inclement weather

Manual handling injury
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR PRECAST CONCRETE FLOORING WORK

Work to be carried out by experienced and competent persons, briefed as to METHOD STATEMENT/RISK ASSESSMENT

Overhead services to be protected, goalposts etc/isolated prior to work commencing.

Delivery route through existing structures to be determined prior to work commencing.

Delivery route through existing structures to be determined prior to work commencing.

SAFETY HELMETS & FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, harnesses and Hi-Vi vests used as required - RISK/COSHH ASSESSMENT MANUAL HANDLING ASSESSMENT to determine method of lifting materials etc.

Firm ground for mobile crane stability, adequate space for crane outriggers and access equipment etc

Cranes (SWL) to safely lift beams etc, to be in good order certificated, weekly inspection on standard report form and operated by certificated (CITB) driver assisted by certificated (CITB) banksman/slinger wearing Hi-Vi vest - Work area to be barricaded to prevent access below and warning signs erected.

Work to cease during inclement weather (high winds)

Lorries to observe speed limit, fitted with reverse alarms and assisted by banksman.

Tail ropes to be used to guide beam into position.


	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	BRICK/BLOCKWORK


	Site activity and condition

Falls of persons and materials

Access and Egress

Head, foot, hand and eye injury

Noise

Manual handling injury

Plant and equipment operations

Exposed fish-tail ties

Other persons incl public

Loading/unloading operation

Splashes

Housekeeping
	JOB SPECIFIC RISK ASSESSMENT FOR BRICK/BLOCKWORK

Work to be carried out by experienced and competent persons, briefed as to requirements of RISK ASSESSMENT

Fully boarded bandstands, scaffolds with guardrails, toeboards and mesh in position if over 2M high.

Fans and debris netting positioned to protect other persons, public etc.

All ladders providing access, correct length and secured 

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, overalls, hearing defenders used as required RISK/COSHH/NOISE ASSESSMENT

Plant and equipment to be in good order, guarded etc (Electrical tools 110 volts only) and covered by a current test certificate.

Cartridge fixing tool operatives to be certificated.

MANUAL HANDLING/JOB SPECIFIC RISK ASSESSMENT to determine method of lifting materials etc.

Work area to be kept clean and tidy, waste removed daily.  All waste to be lowered to the ground NO THROWING (bombing) allowed.

All materials handling equipment to have current test certificate and operated by certificated (CITB) persons

Signs to be erected warning of overhead work.

Replace 'fish tail' type ties with safer alternative.

Exposed 'fish tail' type ties to be covered


	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	CARPENTRY & JOINERY

- Roof trusswork

- 1st and 2nd fix


	Site activity and conditions

Falls of persons and materials

Access and egress

Head, foot, hand and eye injury

Dust and splashes

Noise

Manual handling injury

Plant and MC operations

Other persons incl public

Housekeeping

Loading/unloading operations

Inclement weather
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR CARPENTRY & JOINERY WORK

Work to be carried out by experienced and competent persons, briefed as to requirements of Method Statement/Risk Assessment.

Fully boarded bandstands, scaffold towers, scaffolds with guardrails, toeboards and mesh in position if over 2m high.  Fans and debris netting positioned to protect other persons, public etc.  All ladders providing access, correct length and secured stepladders in good condition.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, overalls, hearing defenders, respiratory protection and harnesses used as required

RISK/COSHH/NOISE ASSESSMENT

MANUAL HANDLING/JOB SPECIFIC RISK ASSESSMENT TO DETERMINE METHOD OF LIFTING MATERIAL ETC.

Work area to be kept clean and tidy, waste removed daily

All waste lowered to ground - NO THROWING (bombing) allowed.

Plant and equipment to be in good order, guarded etc (Electrical tools 110 volts only) and covered by a current test certificate.

Cartridge fixing tool operatives to be certificated.

All materials handling equipment to have current test certificate and operated by certificated (CITB) persons

Warning signs to be erected, warning of overhead work

Work to cease during inclement weather (high exposed elevation)

Tail ropes used to guide trusses into position

Trusses to be braced/secured to prevent collapse.
	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	ROOFWORK

- Felt and Batten

- Tiling, slates etc

- Lightning Conductors

- Services

- Sheet covering


	Site activity and conditions

Falls of persons and materials

Access and Egress

Head, foot, hand and eye injury

Dust and splashes/fumes

Hazard materials eg lead

Manual handling injury

Plant & M/C operations

Nails in timber

Fire/explosion (LPG)

Housekeeping

Other persons incl public

Inclement weather

Loading/unloading operations

Electrocution

Overhead Services
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR ROOFWORK

Work to be carried out by experienced and competent persons, briefed as to requirements of Method Statement Risk Assessment

Fully boarded scaffolds with double guardrails, toeboards and mesh in position if over 2M high.  Debris netting/rescue netting/fans erected to protect other persons/public etc.

All ladders providing access to be secured.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, respiratory protection, overalls, Hi-Vi vest, harnesses used as required - RISK/COSHH ASSESSMENT.  MANUAL HANDLING, RISK ASSESSMENT to determine method of lifting materials etc

Overhead services protected goalposts erected prior to work commencing.

Firm ground for mobile crane stability, adequate space for crane outriggers and access equipment.  Crane SWL to safely lift trusses, materials etc. to be in good order, certificated, weekly inspections on standard report form and operated by certificated (CITB) driver and assisted by certificated (CITB) banksman/slinger.  Wearing Hi-Vi vest.

All timber de-nailed.

Work area to be kept tidy, waste removed daily.

Plant and equipment to be in good order, guarded etc (Electrical tools 110 volts only) and covered by a current test certificate.

All materials handling equipment to be operated by certificated (CITB) persons.
	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	ROOFWORK

Continued


	
	                                               -2-                                      

Cartridge fixing tool operatives to be certificated.

No chain saws allowed on site.

Fire extinguishers positioned adjacent to boilers

Boilers not allowed on roofs.

All LPG cylinders secured in position and away from any heat source (3M).  Hoses in good condition and clipped.

Cylinder draw off capacity to cope with demand without frosting.  All cylinders to be removed from site, end of shift.

Work to cease during inclement weather.

Roof trusses to be braced.

Personal hygiene standards maintained.

Warning signs erected re. overhead work.

Tail ropes to be used to guide trusses into position.

All materials stored at high level to be made secure in position.


	Site Manager

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	MECHANICAL & ELECTRICAL

- 1st & 2nd Fix Plumbing


	Site activity and conditions

Falls of persons and materials

Access and Egress

Head, foot, hand and eye injury

Dust and splashes, fume

Noise

Manual handling injury

Plant & M/C operations

Housekeeping

Loading/Unloading operations

Electrocution

Fire
	JOB SPECIFIC RISK ASSESSMENT FOR MECHANICAL AND ELECTRICAL WORK

Work to be carried out by experienced and competent persons, briefed as to requirements of Risk Assessment.

Fully boarded bandstands, scaffold towers, scaffold with guardrails, toeboards and mesh in position if over 2M high.  Fans and debris netting positioned to protect other persons, public etc

Stepladders in good condition.

SAFETY HELMETS & FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, overalls, hearing defenders

Respiratory protection & harnesses used as required

RISK/COSHH/NOISE ASSESSMENT, MANUAL HANDLING/JOB SPECIFIC RISK ASSESSMENT TO DETERMINE METHOD OF LIFTING MATERIALS ETC

Work area to be kept clean & tidy, waste removed daily

Plant and equipment to be in good order, guarded etc (Electrical tools 110 volts only) and covered by a current test certificate.

All materials handling equipment to have current test certificate and operated by certificated (CITB) persons

Signs to be erected, warning of overhead work.

Fire extinguishers positioned in hot work areas.

Ducts, risers, holes in floors to be either securely covered, fenced and warning notices positioned.

Work area ventilated.

PERMIT TO WORK SYSTEM FOR ALL 'LIVE' ELECTRICAL WORK.

All work areas and any other adjacent area to be inspected one hour after completion of work as a fire precaution after any 'hot work'.
	Contract Manager to obtain from Contractor

Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	COMMISSIONING


	Electrocution

Explosion

Gas escapes
	All commissioning work to be undertaken by competent and experienced person in accordance with the requirements of either a Method Statement or a Permit-to-Work (all high risk work eg. electrical)

No access for unauthorised persons.


	Contractor


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	LIFT WORK

- INSTALLATION

- REMOVAL


	Site activity and conditions

Falls of persons and materials

Head, eye, hand and foot injury

Dust

Manual handling injury

Plant & M/C operations

Housekeeping

Electrocution

Fire

Confined space working

Ventilation

Noise

Services

Other persons incl public
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR LIFT WORK

Work to be carried out by experienced and competent persons, briefed as to requirements of Method Statement/Risk Assessment.

Fully boarded scaffold with guardrails and toeboards in position if over 2m high

Door openings to be secured/barricaded to prevent falls of persons.

Work area ventilated.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection, harnesses, respiratory protection, hearing defenders used as required RISK/COSHH/NOISE ASSESSMENT

MANUAL HANDLING ASSESSMENT to determine method of lifting materials etc

All plant and equipment to be in good order, (Electrical equipment to be 110 volts only) and covered by a current test certificate.

All lifting equipment (SWL) to cope with weight of materials etc, to have current test certificate, weekly inspection on standard report form and operated by certificated (CITB) persons.

All work areas to be kept tidy, waste removed daily

Existing services isolated before work commences.

Fire extinguishers position in all work areas.

Warning notices erected off work in progress.

PERMIT TO WORK on live electrics


	Contract Manager to obtain from Contractor

Contractor

Site Manager




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	PLASTERING

DRYLINING

SCREEDING

RENDERING

CEILING WORK


	Site activity and conditions

Falls of persons and materials

Access and Egress

Head, foot, hand and eye injury

Dust and splashes

Manual handling injury

Plant & M/C operations

Housekeeping

Personal Hygiene
	JOB SPECIFIC RISK ASSESSMENT FOR PLASTERING, DRYLINING, SCREEDING, RENDERING WORKS

Works to be carried out by experienced and competent persons, briefed as to requirements of risk assessment

Full boarded bandstands, scaffold towers, scaffolds level, with guardrails, toeboards and mesh in position if over 2M high.  Stepladders in good condition.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

Gloves, eye protection and respiratory protection used as required - RISK/COSHH ASSESSMENT

MANUAL HANDLING/JOB SPECIFIC RISK ASSESSMENT TO DETERMINE METHOD OF LIFTING MATERIALS ETC

Work area to be kept clean and tidy, waste removed daily

Plant and equipment to be in good order, guarded etc (Electrical tools 110v only) and covered by a current test certificate.

All materials handling equipment to have current test certificate and operated by certificated (CITB) persons

Cartridge fixing tool operatives to be certificated

Personal hygiene standards maintained.


	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	DECORATIONS

- PAINTING

- TILING

- FLOOR COVERINGS

- SANITARY EQUIPMENT


	Site activity and conditions

Falls of persons and materials

Access and Egress

Head, eye, hand and foot injury

Dust, fume and splashes

Personal Hygiene

Housekeeping

Plant & M/C operations

Electrocution

Fire

Manual Handling Injury
	JOB SPECIFIC RISK ASSESSMENT FOR DECORATING WORK

Work to be carried out by experienced and competent persons, briefed as to requirements of RISK ASSESSMENT.

Fully boarded, bandstands, mobile scaffold towers level and equipment with guardrails and toeboards if over 2m high.  Stepladders in good condition.

Work area ventilated.

SAFETY HELMETS AND FOOTWEAR WORN ALL THE TIME

Gloves, eye protection, respiratory protection, overalls used as required - RISK/COSHH ASSESSMENT.

MANUAL HANDLING/RISK ASSESSMENT to determine method of lifting materials etc.

Work area to be kept tidy, waste removed daily.

Personal hygiene standards maintained.

All plant and equipment to be in good order.

(Electrical equipment 110 volts only) and covered by a current test certificate.

Fire extinguishers positioned in all work areas.

Access and egress to be maintained for other site persons.


	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	EXTERNAL WORKS

- LANDSCAPING

- KERB LAYING

- PAVIOURING

- BLACK TOPPING

- DRAINAGE

- CONNECTIONS


	Site activity and condition

Ground conditions

Underground & overhead services

Head, eye, hand and foot injury

Confined space working

Dust, gas, fume and splashes

Noise

Plant & M/C operations

Other persons incl public

Collapse of excavation

Manual Handling injury

Personal hygiene

Fire

Road Traffic
	METHOD STATEMENT/JOB SPECIFIC RISK ASSESSMENT FOR ANY EXCAVATION WORK DEEPER THAN 1.2M FOR CONNECTIONS TO LIVE FOUL DRAINS ETC AND FOR WORK ON THE PUBLIC HIGHWAY

Work to be carried out by experienced and competent persons, briefed as to Method Statement/Risk Assessment

Underground and overhead services to be located, marked protected, isolated prior to work commencing.

Road protection and traffic control movements as per Local Authority/Chapter 8.

Excavations to be adequately supported to prevent collapse with secured means of access, barriers to be erected to prevent falls of persons.

Workplace to be ventilated and tested prior to and during work for oxygen level 20%.  Operatives to be harnessed and attached to rescue line.  Rescue attendant to be present at all times.

SAFETY HELMETS AND FOOTWEAR TO BE WORN ALL THE TIME

Gloves, overall, eye protection, respiratory protection, harnesses, Hi-Vi vest.  Protective clothing, hearing defenders to be used as required.  RISK/COSHH/NOISE ASSESSMENT

MANUAL HANDLING ASSESSMENT TO DETERMINE METHOD LIFTING MATERIALS ETC

All cuts and abrasions to be covered and operatives made aware of Wiels disease and the need for Tetanus.

Signs erected to warn other persons inc public of work in progress.

All plant and equipment to be in good order (electrical equipment to be 110 v only) and covered by a current test certificate.
	Contract Manager to obtain from Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	EXTERNAL WORKS

CONTINUED


	
	                                    -2-                            

Firm ground for mobile lifting equipment stability, adequate space for outriggers and access equipment etc.

Cranes (SWL) to safely lift materials etc, to be in good order, certificated, weekly inspections on standard report form,  operated by certificated (CITB) persons and assisted by certificated (CITB) banksman/slingers.

Banksman to assist reversing lorries which should be fitted with reverse alarm equipment.

Dumper, excavator, roller, drivers to be certificated (CITB) 

Fire extinguishers to be on all blacktopping M/Cs
	Contractor

Site Manager




	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	VEHICULAR MOVEMENT ON SITE

- Site Transport

- Plant and Equipment

- Delivery, lorries etc


	Vehicular accidents

Pedestrian accidents

Speeding

Tipping over
	Vehicle access will be defined, signposted and where necessary illuminated to protect pedestrian movements on site.

A maximum speed limit of 10mph will be enforced.

All vehicles must be in good working order, receive regular maintenance and daily checks and inspected to comply with any statutory requirement - all inspections must be recorded on the standard report form.

Contractors before using any vehicle on site must ensure a copy of recent test and examination is given to the Site Manager.

All drivers must be in possession of a full driving licence, a certificate of competency and report medically fit for work.

All vehicles to be used/operated to within their design limits.

Vehicles discharging exhaust fumes must not operate in confined space work areas.

Vehicles not in use must be either removed from site or parked securely in designated parking areas.

Banksman wearing hi-vi clothing to assist all vehicles reversing and other manoeuvres where required.

Bases of scaffolding, ladder accesses, manholes, access to excavation to be protected by physical barriers to prevent vehicle accidents and vehicles tipping over.


	Site Manager

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	MECHANICAL PLANT AND EQUIPMENT


	Misuse by operatives

Noise

Fume

Tripping hazard - cables and hoses

Breakdown
	Contractors to ensure all mechanical plant and equipment is in good working order suited for the task of work and used/operated by competent certificated operator/drivers.

Contractors must ensure that before using mechanical plant and equipment a copy of recent test and examination is given to Site Manager.

Contractors before using mechanical plant and equipment must ensure its position does not pose a risk to other site users, client and public etc by keeping noise, dust, fume, vibration, splash and residue to a reasonable level of acceptance.

Plant and equipment which emits exhaust fume, to vent to atmosphere and must not be positioned in a confined space.

Operatives likely to be exposed to noise levels above 85dBA to wear hearing protection as required by any NOISE ASSESSMENT

Hoses and cables to be positioned securely to prevent tripping hazard.

Where supplied by the Principal Contractor to be used by a number of contractors, its use will be controlled by means of a rota system or similar.

All plant and equipment when not in use will be either removed from site or securely stored awaiting further use.

All plant and equipment to be maintained in good working order and any repair carried out by competent persons.


	Contractor

Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	WASTE
	Accumulation

Contamination

Pollution

Personal Hygiene

Fire
	Contractors are responsible to ensure that all waste associated with their work is removed on a regular basis to waste bins or skips.

Contractors must ensure that no waste is allowed to pollute any water course, drain, gully etc.

All waste including contaminated waste to be removed from site by a licensed waste removal contractor and delivered to a licensed waste site.

All operatives handling contaminated waste will use/wear PPE as per COSHH Assessment.

Fire extinguishers to be positioned adjacent to any area where combustible waste is stored.

All waste will be removed from site on a regular basis.


	Contractor

Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	PROVISION AND USE OF TEMPORARY SERVICES 

eg Electricity


	Electrocution

Trailing Cables

Fire

Overloading
	Temporary electrical supply to cater for all site requirements.

All electrical installation and repair work to be carried out by a competent electrician in accordance with statutory requirements and the IEE Regulations.

All electrical cables and transformers to be routed away from traffic and pedestrian access where reasonably practical.

All electrical cables to be secured, highlighted and protected - armoured cable to be used on external runs and to transformers.

Temporary electrical switchgear to be secured against unauthorised access and signposted with warning signs.

All electrical installation work to be inspected weekly.

All site huts, offices etc to incorporate means of tripping to prevent persons being electrocuted.

All temporary electrical supply on site will be transformed down to 110 volts.

All waste etc to be removed regularly from all electrical installation, transformers etc.


	Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	ACCESS AND EGRESS TO ALL AREAS OF WORK


	Trips of persons

Slips of persons

Falls of persons

Vehicle accidents
	Access to all work areas will be established, maintained, illuminated and signposted to ensure the safe access and egress of all site users, visitors etc.

All pathways, gangways, staircases, access points to ladders, hoists etc will be level, kept free of waste, spillage, materials and regularly cleaned.

Ladders providing access to be in good condition, correct length, set at the correct angle and secured in position.

Protection on staircases to be secured in position.

Pedestrian access to be separate from vehicle access where reasonably practical.

Warning signs to be posted with regard to pedestrians.

All temporary run-ups to be of adequate design and construction to withstand loading and to be at least 2 scaffold boards wide.  Any run-ups exceeding a rise of more than 1.5:1 to have laths of similar to prevent slips of persons.

All run ups onto ladders, skips, stacks of material are not permitted.


	Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	STORAGE

- Materials

- Waste

- Plant and Equipment


	Stacking of materials

Fire

Spillage

Falls of materials

Cross contamination
	Storage areas to be clearly defined by notice.

All materials, waste, plant and equipment to be securely stored, brick and block packs no more than 2 high, drain pipes etc to be chocked.  

All storage areas to be level, free of debris and receive regular cleaning.

All pallets to be inspected for good order - broken pallets will not be permitted on site.

Highly flammable liquids and LPG to be stored in purpose designated storage areas together with fire precaution signs and extinguishers.

All materials, waste, plant and equipment will be segregated in storage to prevent cross-contamination.

Storage containers will be maintained in good order and any material, plant and equipment stored within will be in a neat and tidy order.

All spillages to be dealt with as per COSHH assessment.

Diesel/Fuel tanks to be binded to contain spillage.


	Site Manager


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	STORAGE OF MATERIALS AT HEIGHT


	Falling materials

Personal injury - crashing striking etc

Collapse of scaffolding
	On all scaffolding above 2 metres high where material is to be stored awaiting use then a brickguard or similar mesh must be in position on all working lifts, with close sheeting/debris netting positioned to give additional protection.

Material stored on scaffold must be adjacent to uprights and not exceed the toe-board if brickguards/mesh or similar are not provided and not exceed the height of the guardrail under any circumstances.  Where practical all stored material should be secure in position and at least two boards plus be maintained to allow safe access and egress for site operatives.

Additionally, close boarded fans should be erected and positioned above access points or adjacent to areas where the public or other site users are to pass below.

Scaffold to be structurally sound to take the weight of stored material.

Materials craned over the site, public areas etc. to avoid persons as is resonably practical.

All persons below craned materials to wear safety helmets.

No material to be stacked adjacent to any excavation.  

No material to be thrown from scaffolding, all material to be lowered.

Temporary work platforms eg bandstands/trestle must be set level on ground free of debris, fully boarded and not overloaded.

All mobile scaffold towers must be free of materials etc before being moved to another position.


	Site Manager

Site Manager

Contractor

Contractor


	ACTIVITY
	HAZARD AND RISK
	CONTROL ACTION
	DELEGATION

	DISTRIBUTION OF MATERIALS


	Weight, size and shape of materials

Manual handling injury

Falls of materials

M/C accidents
	Materials that cannot be manually handled safely, will be delivered to areas of work by mechanical lifting equipment eg. cranes, fork lifts, dumpers, excavators, hoists etc.

All mechanical lifting equipment must be in good working order, receive regular maintenance, daily inspections and weekly inspections which must be recorded on the standard report form.

Contractors supplying and using mechanical lifting equipment must give the Principal Contractor a copy of recent test and examination before use.

Driver/Operators of lifting equipment must be competent certificated and report medically fit for work.

Crane forks to be netted to prevent falls of materials.

Lifting of materials to be in accordance with technical advice from manufacturers/suppliers.

Materials awaiting to be used to be securely stored as near as possible to the area of work.

All manual handling will be in accordance with a job specific MANUAL HANDLING ASSESSMENT.

The HODDING OF MATERIAL UP OR DOWN LADDERS WILL NOT BE PERMITTED.


	Site Manager


General Safety Plan/Risk Assessment


