


Details for Proposed works to fit new railings and gate
The new railing will be fixed to the existing plinth.  The new railings will use the existing holes left by the original railings as their fixing points (12 cm apart). The old hole points are to be drilled out and the new railings resined in with 5 star resin grout. 

Details for Proposed work to pathway and step
We wish to have the entire garden at the same level. We therefore propose moving the step up forward from its current position, inside the garden, to the gate. The area between the gate and the existing step up is to be filled with concrete to a height of 18cm (this work is already underway). This height matches the existing pathway so that there will be a smooth connection between them for the tiles which are to be laid on top. The area to be filled with concrete is about 1sqm.  The entire of the hard surface of the front garden, including this newly raised area, will then be covered with Victorian Tiles with a depth of 12mm. 

The new step up will be finished off to the front with a new stepping stone. The stepping stone will be in complete alignment with the existing plinth in terms of width and height. The stone's specifications are as follows: Darleymoor Buff Sawn Yorkstone which is a sandstone, very similar in appearance to the existing plinth.

[bookmark: _GoBack]The above information is taken from emails sent by the applicant to the Case Officer on 25th April 2018 and the 26th and 27th June 2018.




 


 


Details for 


Proposed works to fit new railings and gate


 


The new railing will be fixed to the exi


sting plinth.


 


 


The new railings will use the existing 


holes left by the original railings as their fixing points (12 cm apart).


 


The


 


old hole points 


are to be


 


drilled 


out and the new railings


 


resined 


in 


with 5 star resin grout.


 


 


 


Details for 


Proposed w


ork to pathway and step


 


W


e 


wish


 


to have 


the entire


 


garden at the same level. 


We therefore propose


 


moving the 


step


 


up


 


forward


 


from 


its current position


,


 


inside the garden


,


 


to the gate. 


The area 


between the gate and the existing step up is to


 


be


 


filled with concrete to a height of 


18cm (this work is already underway).


 


T


his 


height


 


matches the existing pathway so that 


there


 


will be 


a smooth connection between them for the tiles


 


which are to be laid on 


top


. The area


 


to be filled with concrete


 


is about 1sqm. 


 


The entire of the hard surface of 


the front 


garden


, including this newly raised area,


 


will then be covered with Victorian 


Tiles with a de


p


th of 12mm.


 


 


 


T


he new step


 


up


 


will be finished off to the front with a new stepping stone. T


he 


stepping stone will be in complete alignment with the existing plinth in terms of width 


and h


e


ight.


 


T


he stone's specifications are as follows: Darleymoor Buff Sawn Yorkstone 


which is a sandstone, very similar


 


in appearance to the existing plinth.


 


 


The above information is taken from emails sent by the applicant 


to the Case Officer 


on 


25


t


h


 


April 2018 and 


the 26


th


 


and 27


th


 


June 2018.


 




    Details for  Proposed works to fit new railings and gate   The new railing will be fixed to the exi sting plinth.     The new railings will use the existing  holes left by the original railings as their fixing points (12 cm apart).   The   old hole points  are to be   drilled  out and the new railings   resined  in  with 5 star resin grout.       Details for  Proposed w ork to pathway and step   W e  wish   to have  the entire   garden at the same level.  We therefore propose   moving the  step   up   forward   from  its current position ,   inside the garden ,   to the gate.  The area  between the gate and the existing step up is to   be   filled with concrete to a height of  18cm (this work is already underway).   T his  height   matches the existing pathway so that  there   will be  a smooth connection between them for the tiles   which are to be laid on  top . The area   to be filled with concrete   is about 1sqm.    The entire of the hard surface of  the front  garden , including this newly raised area,   will then be covered with Victorian  Tiles with a de p th of 12mm.       T he new step   up   will be finished off to the front with a new stepping stone. T he  stepping stone will be in complete alignment with the existing plinth in terms of width  and h e ight.   T he stone's specifications are as follows: Darleymoor Buff Sawn Yorkstone  which is a sandstone, very similar   in appearance to the existing plinth.     The above information is taken from emails sent by the applicant  to the Case Officer  on  25 t h   April 2018 and  the 26 th   and 27 th   June 2018.  

