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Extension to rooftop walkway
The existing walkway does not meet ne Health & Safety regulations for providing access to service the chillers that are sited on the roof of the Huntley & Palmer Gallery. The existing walkway does not provide safe passage to all the areas surrounding the chiller and has also been partially removed following some alterations to ventilation system, This new walkway will meet the Health & Safety requirements and provide safe access to all parts of the working area around the chiller. This will also provide access to guttering that has been previously inaccessible. The walkway is to be manufactured from open mesh flooring (Lionweld Kennedy). 

The walkway will be supported by means of purpose made steel frames that are fixed to the existing supportive steelworks and the existing flank wall.

The walkway overlooks an internal courtyard that is not accessible to the general public (other than as a fire exit route). The courtyard is visible from inside the building, but hidden from view by use of blinds.
The chiller requires regular maintenance and is essential to providing a constant ambient atmosphere to protect the valuable artefacts contained within the museum.
