Revised Method of installation:
•	Assess the ground levels and visually check for roots.
•	The area would be marked out to the correct size and shape.
•	A geotextile membrane would be laid directly on the ground.
•	A layer of soft sand would be placed on top of this membrane to cushion the roots and absorb root expansion.
•	A damp proof membrane would be laid on top of this sand to protect the roots and surrounding ground from the concrete.
