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SAP Summary Overview Report
Project Ref: 2no. new dwellings at 1a Eaton Place 
SAP Type: New Build Part L 2021


This document must be submitted with your SAP calculations for building control approval

	Building Fabric

	Element
	Construction build up including insulation & thickness
	U value (W/m2K)

	Ground floor

	75mm screed, 150mm Kingspan (0.019), 100mm concrete

	0.11

	Exposed floor
	50mm screed, 200mm concrete, 130mm Rockwool Soffit slab
	0.25

	External wall 
	100mm brick, 10mm cavity, 90mm Kingspan (0.019), 100mm lightweight 7n block (0.018), plasterboard on dabs

	0.17

	Ceiling
	300mm mineral wool above joists, 100mm mineral wool between joists, plasterboard
	0.11

	Windows 
	  Double Glazed (unit U-value including frame and glazing) G-value 0.66
	1.40

	Solid Front Door
	(unit U-value including frame and glazing)
	1.20

	Air test
	Design target 4.00
	 4.00 m3/hm2

	Thermal bridging
	Recognised Construction Details.  Copy of relevant checklists can be found here
	Y-Value

	
	PLEASE NOTE: For calculated / bespoke psi value details to be used in the SAP Calculations (L1A ONLY) the thermal Junction checklist guidance MUST be implemented on site. Failure to adhere to these standardized junction details will require the use of default PSI values for the junction heat loss which will adversely affect the performance of the dwelling(s) against Part L. If you cannot meet the requirements of the ACDs or the construction changes, please inform us at the earliest stage so compliance can be achieved before the project progresses.
	

	HVAC

	Type
	Specification
	

	Primary heating
	Electric panel heaters
	%
Efficiency

	Secondary heating
	 N/A
	

	Emitter
	Panel heaters
	

	Primary heating Controls
	Programmer & appliance thermostats
	






	DHW
	Dimplex EDL170 hot water heat pump
https://www.dimplex.co.uk/products/heat-pumps/hot-water-heat-pumps?gad_source=1&gclid=EAIaIQobChMIku7LjPm4jAMVUZhQBh1u2whwEAAYASAAEgJ1nPD_BwE

	
kWh/day

	Ventilation
	Intermittent extract fans to all wet rooms
	2

	Lighting
	100% low energy light fittings throughout including external lights.
Minimum 75 lumens per circuit watt
	100%

	Solar Hot Water
	N/A
	

	Photo Voltaic panel
	N/A

	

	DISCLAIMER: Please note that the design inputs outlined above are key to the project's compliance with Part L1A/L1B of building regulations. Should any of the details above not accurately represent the proposals of the project or if any of the measures above cannot be incorporated for any reason, please let us know, as the project may fail the regulations. If changes are made to the above specification without contacting us, and the project fails there will be a consultation fee charged to help ensure the building passes the relevant regulations

	Client/contractor Signature: 
	Date: 







	Plot
	EPC Rating

	GF
	80 C

	FF
	73 C
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