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Examples of current site conditions:
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This section will replace a 6”
with 140mm PE by way of
dead insertion. All meter

boxes are to remain in tact in

their current positions as the
intention is to insert back

from the main to the meter.
No Trees will be affected.
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This is a 6” section being
replaced with 90mm PE.
Will be live transferred. We
have surveyed meter
locations and confirmed

they will remain in situ as we
can insert back. Trees will
not be affected.
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This section of 4” will be

replaced with 75mm PE by
way of insertion. The
intention is to push all
services back to their
current position. No Trees
will be impacted in this
section.
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This section of 6” is being
replaced with 90mm PE
which will allow for easy

live insertion. No services

or trees are being affected
in this area.
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6: Mater Box No.
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Figure 1: House Entry Tee Ground Floor No. 28 Figure 2: House Entry Tee Ground Floor No. 41




image1.png
4”To be replaced with
72mm PE by insertion.
Services to be inserted

back. No impact on
Trees.
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6” Section being replaced
with 140mm by insertion
PE - All services to be
inserted back. The tree in
the image will not be
affected as we are
inserting. Any connection
holes will be dug away
from this area.





