
	
Arboricultural Method Statement
Arboricultural Implications Assessment


SITE ADDRESS      18 Rosehill Park Emmer Green Reading   Rg4 8XE


1.0	Arboricultural Method Statement Methodology. 

1.1	The Arboricultural method statement provides the means by which areas of construction near to the Root Protection Area (RPA) of retained trees can be achieved whilst minimising the impact of construction activity on nearby trees.


1.2	The excavation of foundations for any structure on sites where trees are present may result in root damage due to the position of machinery and builders materials  Where root loss is likely to occur, it is important that a method of construction that minimises the impact on tree roots is utilised.

 
2.0	Tree Protection Measures
2.1	The tree is in the garden of the neighboring property are shown on the plan and it should be noted that the proposed excavations are not within the RPA. 
2.2	Heras fencing is however proposed and indicated on the plan, and this must be erected before any works commence and kept in position throughout the construction process. As soon as the work is complete and all leftover materials carted away the railing can be taken down and removed from site. 

3.0       PROVISION OF CAR PARKING SPACES AT THE FRONT 

	Effects of addition two parking bays on immediate Landscape 

3.1       The corner of the site where the new parking bays are proposed (noted on the plan) has a Common Yew and Japanese Meadow Sweet that are currently in direct competition due to their close proximity and appear to be suffering as a consequence.

The remainder of the front garden has a generous number of shrubs however it could be argued that there is too many for such a small area and some thinning would be recommended to enhance growth (the proposes car parking does not affect this work) 

It is proposed, if possible, to re locate the two affected bushes at the rear in early October if possible however if this is not possible for either time or physical constraints two additional similar plants will be provided at the rear to mitigate the loss at the front. 
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