Wantage Hall Tree Work Requirements
	No.
	Species
	
	Works required
	Reasons for work
	
	Map

	02FB
	Yew
	
	Lift Crown to achieve 3m over foot path Remove epicormic growth to 2m
	Statutory clearance
	
	Map 1

	02FE
	Horse Chestnut
	
	Lift crown3m over foot path 6m over carriage way
	Statutory clearance
	
	Map 1

	02E3
	Horse Chestnut
	
	Fell to 1m
	Trunk decay which has resulted in crown failure during the summer
	
	Map 1

	02DH
	Arbutus unedo
	
	Lift crown to 3m over foot path
	Statutory clearance
	
	Map 1

	02DJ
	Norway Maple
	
	Lift crown to 2m
	Facilitate site usage
	
	

	02DK
	Lime
	
	Lift Crown to 3m
	Facilitate site usage
	
	Map 1

	02DL
	Lime
	
	Lift Crown to 3m
	Facilitate site usage
	
	Map 1

	02DM
	Robinia
	
	Remove dead wood reduce lateral east to give 2m clearance from building
	On-going crown management/ Site safety
	
	Map 1

	02EA
	Robinia
	
	Remove dead wood
	Site safety
	
	Map 1

	02EB
	Lime
	
	Lift Crown to 3m
	Facilitate site usage
	
	Map 1

	02EC
	Lime
	
	Lift Crown to 3m
	Statutory clearance
	
	Map 1

	02ED
	Lime
	
	Lift Crown to 3m
	Facilitate site usage
	
	Map 1

	02EE
	Lime
	
	Lift Crown to 3m
	Facilitate site usage
	
	Map 2

	02EF
	Lime
	
	Lift Crown to 3m
	Facilitate site usage
	
	Map 2

	02E5
	Lime
	
	Lift Crown to 3m
	Facilitate site usage
	
	Map 2

	02E6
	Lime
	
	Lift Crown to 3m
	Facilitate site usage
	
	Map 2

	02E7
	Lime
	
	Lift Crown to 3m
	Facilitate site usage
	
	Map 2

	02EK Group
	Sycamore Cherry Plum, 
	
	Fell squirrel damaged Sycamore cut back over hang to achieve 5m clearance from building
	On-going management 
	
	Map 2

	02EW
	Turkey Oak
	
	Remove hanging branches
	Site safety
	
	Map 2

	05M3
Group
	Sycamore, Turkey Oak
	
	Select trees for retention remove competing seedling trees and vegetation 
	On-going management
	
	Map 2

	05ES
	Turkey Oak
	
	Remove lowest 2 branches
	Formative pruning
	
	Map 2

	04U8
	Leyland Cypress Hedge 
	
	Reduce width to kerb line reduce height to approximately 6m just above previous pruning points
	Facilitate site usage
	
	Map 2

	02F7
	Field Maple
	 
	Remove dead wood Reduce upper crown 2-3m to encourage retrenchment
	Site safety/ On-going management
	
	Map 1

	02FB
	Walnut
	
	Fell to ground level
	Honey Fungus
	
	Map 1



