Window Replacement 
Information supporting Listed building Consent Application

General: Grade II listed Coachhouse originally built circa 1750
12 The Brookmill, Coley Park Farm, RG! 6DD

Existing:
· Developed in  June 1986
· Front of Property:
· Existing Description
· 3 large archways at front of property, 2 of which were turned into windows, one turned into a porch. This note applies to the windows only
· None of the windows are original
· Some original wood remains in central archway but not the windows
· Dimensions and condition:
· 2 times 250cm wide x 250cm high to lowest point.. extra 15 cm to top of arch. Wood beyond repair
· Middle archway 2.85 m wide – top wood plank beyond repair/ fallen. To be replaced like with like
· Rear of Property
· Existing Description
· 2x windows RHS and LHS at Ground floor level
· Patio/French doors/windows combined unit at Ground floor level
· 3 windows on first floor. RHS and LHS the same size. Central window larger
· Dimensions and condition:
· Ground floor
· RHS and LHS ground floor 135 cm high x 90cm wide
· Middle patio door/window 246cm wide x 210cm high
· First floor
· RHS and LHS 90cm wide x 115 cm high
· Central window 120cm wide x 130cm high
· All windows and French door /patio unit timber beyond repair

Proposed:

· Windows for front of Property:
· Proposed material: timber Iroka and Accoya timbers. 
· Proposed double glazing: All glazing would be Heritage standard clear toughened low E Argon filled with furniture line stamp finish. Thick profile, 4-16-4mm thickness
· Proposed colour: Black
· Other detail: 4 evenly spaced panes, non-opening, to match existing, clear glass, spacer bar to be black to match window frame colour. All existing detail will be replicated

· Windows for rear of property
· Proposed material: timber – finger jointed redwood
· Proposed double glazing: slim profile, 4-10-4 mm for windows RE 1,2,3,4 and 6 (see below). Thick profile 4-16-4  thickness for French/ patio door unit RE 5 (see below)
· Proposed colour: White/ off white
· Other detail: openings to match existing, clear glass, spacer bar to be white to match the colour of the window frames, all existing detailing would be replicated. External patio door to handle to be kaba style bronze.
 

Front Elevation Existing:Middle archway 2.85m wide. Top wood plank beyond repair/ fallen



[image: A building with a clock on the side

AI-generated content may be incorrect.]RHS arched window (FE 2) 250cm W x 250cm H. Single glazed. wood beyond repair
LHS arched window (FE 1) 250cm W x 250cm H. Single glazed. wood beyond repair











[image: A window with blue curtains

AI-generated content may be incorrect.]LHS Arched window FE.1:

Sill failed. 
All wood beyond repair 
Single glazed Softwood 1986



[image: A car parked next to a window

AI-generated content may be incorrect.]RHS Arched window FE. 2:
Sill failed. 
All wood beyond repair 
Single glazed Softwood 1986




[image: A brick building with a arched doorway

AI-generated content may be incorrect.]Central Archway
Some original wood remains. Top left crescent requires replacement. 
Original sill beyond repair, fallen and requires replacement.





Rear Elevation Existing:

[image: A brick house with a few windows

AI-generated content may be incorrect.]Ground floor Central patio door/  casement window arrangement softwood (RE 5) 
Ground floor RHS standard casement softwood window (RE 6) 
Ground floor LHS standard casement softwood window (RE 4) 
1st floor RHS standard casement softwood  window (RE 3) 
1st floor LHS standard casement softwood window (RE 1) 
1st floor Central standard casement softwood  window (RE 2) 











[image: A brick building with a window

AI-generated content may be incorrect.][image: A window on a brick wall

AI-generated content may be incorrect.]LHS RE 1	Central RE 2
Single glazed	Single glazed
Casement	Casement
Softwood 	Softwood







[image: A brick building with a window

AI-generated content may be incorrect.]RHS RE3
Single glazed
Casement
Softwood





LHS RE 4	RHS RE6
[image: A window on a brick wall

AI-generated content may be incorrect.][image: A window on a brick wall

AI-generated content may be incorrect.]







Central Patio door arrangement RE5
[image: A white door with glass panes

AI-generated content may be incorrect.]
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