Design and Access statement

House Overview
SURLEY ROW 1. 5128 (West Side) Caversham Grove (Now Highdown School, Emmer Green) SU 7176 5/287 II GV 2. C18, altered and extended 1878-80 by Richard Norman Shaw in Queen Anne style. The main (older) part: 2 storeys and attic over segmental-headed windows. Red brick with stucco string at 1st floor level, flanking brick piers with rusticated bands. Stone moulded eaves cornice. 5 bays, glazing bar sashes with bracket cills centre 1st floor blind. Door and porch in centre probably by Norman Shaw, with moulded cornice and eared rubbed brick entrance. Tiled hipped roof with gabled dormers (part of Norman Shaw's work). Interior: richly panelled and with lavish plaster enrichments to ceilings (again probably by Norman Shaw). Stone staircase in central well with richly carved eared doorways, panelling and bold modillion cornice. The 1878-80 extensions by Norman Shaw almost, double the house in size. 2 storeys. Red brick. Queen Anne style. with fine garden front to south with loggia, interior decorated in 'Adam' style. Irregular plan with 2 storey gatehouse to stable yard projecting to east. Casement windows with glazing bars. The Norman Shaw work is important as an early example of his Queen Anne revival and some of the interior details in the original (early C18) house are very faithful replicas of that period.

Painting the Manor House stone staircase from the ground to the first floor only
The existing internal staircase for the Manor House forms an original feature and unchanged for the Manor House since being built in the 1800. These steps are made of stones and have a shallow draft. 
Over years these have worn, with the school use this wear has increased further and slip incidents have increased. 
 
We wish to paint the top section of the steps with an Anti-Slip paint in Grey, the main flag stones will be left untouched and therefore will retain their original colour and finish. We hope to use Leyland Trade 5Ltr slate semi-gloss anti slip floor paint is a tough and durable solvent-based coating designed for interior concrete, steel, and wooden floors. This high-performance floor paint features a light aggregate, providing slip-resistance for busy workshops and garages. It delivers a smart slate grey semi-gloss finish. 
 
