	Material
	Manufacturer
	Selection reason and brief

	Primer to deck and upstands if required by system manufacturer

	Fixer AVCL Primer
	Part of the manufacturers system that we are using to ensure the 20 year guarantee

	Self adhesive Vapor control layer 

	Fixer AVCL vapor control layer
	As above

	Flat board insulation, to meet current building regulations requirements of 0.16 W/m²K. Fixed to
VCL using PU adhesive. (Typically around 140mm insulation)

	IKO enertherm PIR insulation board 150mm as required by BREGS
	To meet the required BREGS

	Underlayer felt (Torch on or self adhesive)

	Fixer SIG Sg100816
	20 year manufactures guarantee

	Mineral faced B Roof(t4) cap sheet (Torch on or self adhesive)

	Fixer SIG SG100G35
	As above

	Felt system to be applied strictly in accordance with the manufacturers instructions.

	20 years fixer torch on system
	20 year manufactures guarantee



