CONSTRUCTION NOTES


1. FOUNDATIONS:- See section on plan
2. D.P.C:-Polymer type of d.p.c’s to all walls min 150 above ground level. Thermabate insulated d.p.c. or similar to all reveals in accordance with manufacturers specification .D.p.c. to lap with d.p.m. min 50mm and be continuous with existing. Window frame to overlap cavity closer by 30mm.

3. FLOOR SLAB:- see sction on plan
4. EXTERNAL WALLS:-225 Face brickwork to match existing 
5. PITCHED ROOF:-Concrete interlocking roof tiles to match existing, on battens on Tyvek Supro breathable felt on  trussed rafters to BS 5268 Pt3 1985. Wall plate strapped to wall with 30 x 5  galvanised m.s. straps at 2000 max ccs fixed to 6no. brick courses. 
6. LATERAL RESTRAINT:-30 X 5 m.s straps @ 2000 max ccs to walls parallel to roof and floor timbers.

7. LINTELS:-IG  L1/S 75  lintels over all openings unless stated. R.C. lintels in walls over drains and all voids filled with vermin proof material and compressible sealant and have concrete  cover and surround as necessary
8. S.W. DRAINAGE:-100 diam ½ round pvc gutters to extg system, or 69 diam RWP’s to 100 diam UPVC drain surrounded in 150 pea shingle at 1 in 40 fall to soakaway min 5m from building. Soakaway to be filled with washed rejects to a level 150mm above the invert of the highest incoming pipe and cover with 1000 gauge poly sheet. Cast a 100mm concrete slab over and build up to adjacent levels with topsoil in accordance with BRE Digest 365. 
9. PART P:- All electrical work required to meet the requirements of Part P (electrical safety) will be designed, installed, inspected and tested by a person competent to do so, ie Part P certified. Prior to completion the Council should be satisfied that Part P has been complied with. This may require an appropriate BS 7671 electrical certificate to be issued for the work by a competent  electrician registered with NAPIT, ELECSA, NICEIC or equivalent.   
10. GENERAL:- Builder to check and verify all dimensions prior to works commencing on site. Builder to locate all drains in vicinity of proposal and ensure neither they nor building operations adversely affect each other. This plan is prepared for the sole purpose of seeking L.A. consents. All works to be in accordance with accredited construction details for Part L.   
