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DESIGN & ACCESS STATEMENT

in respect of constructing a new house at
Rear of 92 Whitley Street, Reading, Berkshire RG2 0EQ
1. ENVIRONS
The site is located in south Reading on Whitley Street, a continuation of Basingstoke Road and one of the main routes from the town centre southwards towards Acre Road and other industrial estates, to the Madejski  Stadium and to Hampshire beyond.  Christchurch Road links it to Reading University and the health centre in Northcourt Road.  
The site lies behind commercial premises at Nos.90 and 92 Whitley Street and at the end of a terrace of two-storey residential dwellings on the south side of Essex Street.  Whitley Street itself comprises a bustling commercial centre supported by Essex Street and the many similarly residential streets surrounding it.  There are also schools, places of worship, educational and health establishments close by, many within walking distance, including sports facilities at Cintra Park.
2. THE SITE

The rear of No.92 currently contains a two-storey building, its ground floor having been previously used as a plant room to the existing laundrette at the front of No.92 but now redundant as such, and its first floor currently being used as a residential flat.  This building directly abuts and is set forward of the end-of-terrace house at No.1 Essex Street and, along with the other houses in the terrace, is generally of traditional construction with loadbearing brickwork surmounted by pitched slated roofs.  This two-storey building at the rear of 92 Whitley Street is conjoined to the single-storey neighbouring commercial premises at No.90.
Along the western boundary of the site is a nom.2.0m wide right of way enabling the occupiers of No.94 Whitley Street access to Essex Road.

The ground floor of No.90, which is under separate ownership, projects nom.1.0m beneath the upper storey of the building on site, in effect making it a ‘flying freehold’ 

The entrance to the two-storey building on site is located at the back of the pavement in Essex Street, and there is a small open area between the single-storey front laundrette and two-storey rear residential part of No.92.  The ground floor of the latter has a low ceiling which renders it impractical for most uses other than as a plant room but, as it is no longer needed as such, it has become redundant.
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3. PREVIOUS APPLICATION

In 2020 formal  pre- application advice was obtained from the local planning authority, ref: 200698/PREAPP, for the construction of a 2 bedroom maisonette above a single-storey studio flat.  It concluded that the principle of development was accepted, but raised concerns about overdevelopment and the impact of that design upon the character of the surrounding area.  The advice suggested that a scheme proposing a two-storey dwelling may have some potential, but went on to recommend that the one-and-a-half storey height to match the existing building ‘unless a more appropriate design approach is adopted which does not cause any significant harm to the adjoining terrace.’  It went on to recommend that a full planning application should be ‘limited to a single dwelling ...’ and that ‘The number of bedrooms proposed should comply (as a minimum) with the Nationally Described Space Standards.’
4. CURRENT PROPOSALS
Therefore the applicants propose to demolish and replace the existing one-and-a-half storey building with a new dwellinghouse to provide an improved standard of residential use.  
It is proposed to leave a generous 3.0m gap from the end-of-terrace No.1 Essex Street and to construct a three-storey 3-bedroom 4-person house.  The side gap include the right-of-way to the rear of No.94 Whitley Street, and provide amenity space for the new development, but it would also immediately improve the aspect from 1 Essex Street, relieving it of being overshadowed, and provide a punctuation between the single storey commercial premises in Whitley Street and the two-storey houses in Essex Street, but without dominating either.
The requirements of the Technical Standards have been satisfied in the design:-

-gross floor area = 92.7m2 [min:90m2 required for a 3-bedroom 4-person house]; 

- double bedroom (2): 13.3m2 [min. 11.5m2] and is 2.9m wide [min. 2.75m];

-single bedroom (1): 8.9m2 [min.7.5m2] and is 2.7m wide [min. 2.15m]; 

-single bedroom (3): 10.0m2 [min. 7.5m2] and is also 2.7m wide.
The site is considered too small to provide on-site car parking but, as described above, it is well served by public transport routes and is within walking or cycling distance of a number of commercial, educational, religious and health facilities.
Aspects from the main habitable rooms include over the flat roof of the commercial single-storey No.92.  In any event, windows serving the first floor of No.94 Whitley Street overlook this same roof, which must therefore be kept at that level.
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5. ACCESS

5.1 Specific Access Issues

The proposed development is situated on a broadly level site that is unlikely to provide unusual difficulties for those with mobility problems.   
The pre-application advice specifically required clarification as to how the retail units at No.90 and 92 Whitley Street are currently serviced. However, neither No.90 or No.92 have significant servicing requirements likely to affect transport matters, No.90 being a hairdressing salon with no existing rear access anyway, and No.92 being a launderette which has no over-riding need for the existing rear access that would be removed by the proposals.
5.2 Access from Existing Transport Network

The site lies a short distance from public transport links to commercial facilities in Reading town centre and all destinations in all directions, and is within walking and cycling distance of local commercial, religious, health, educational and social establishments. 

5.3 Access Points and Layout

The new house will only be accessed from Essex Street using the gap between the new house and its neighbour at No.1 Essex Street.
5.4 Maintenance of Access

The access point will be paved with robust materials requiring minimal maintenance.

6. DESIGN

6.1 To provide good quality self-contained residential accommodation in accordance with the Council’s policies and the nationally adopted Technical Standards that seek to maintain standards of residential accommodation while restricting impact upon public resources;

6.2 To provide good quality accommodation that is affordable for key workers in the borough in accordance with its Core Plan.  
6.3 To maintain the prevailing relative residential density in the immediately surrounding area;

6.4 To respond to government policy seeking to better utilise underused urban sites;

6.5 To bring an existing site into improved economic use without undue detriment to its surroundings, thereby maintaining the quality of the surrounding area in a sustainable way and in the long-term public interest.

7. INFRASTRUCTURAL CONTRIBUTIONS

It is anticipated that a contribution will become due for affordable housing off-site of 5% of the market value of the new house based on the formula published in the council’s ‘Supplementary Guidance for Affordable Housing’.
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