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Schedule of External Wall Materials
This schedule should be read in conjunction with the General Arrangement Floor Plans, Elevations and Window & Door schedule along with the Construction Specification
Samples availabe on site.
						
	Item
	Proposed Specification
	Comments
	Image SAMPLE

	External Wall – Main Construction Build-Up

	Brickwork (main)


	Forterra – Wentworth Mixture Brick

Standard Grey Mortor

	
	

	Brickwork (Textured area)
	Forterra – Wentworth Mixture Brick

20mm indend and protrusion

Standard Grey Mortor

	
	[image: C:\Users\alex.kimber\AppData\Local\Microsoft\Windows\INetCache\Content.Word\textured brick shadow.jpg]

	Brickwork (core entrances)
	Synthesis S17 From MBH PLC

Standard Grey Mortor



	
	[image: ]

	Timber Boarding (to community building)
	Kebony Cladding
	
	
[image: C:\Users\alex.kimber\AppData\Local\Microsoft\Windows\INetCache\Content.Word\kebony.jpg]

	Balcony feature fins
	Keybony Timber Fins

Balcony rails (cira. RAL7016)

	
	[image: C:\Users\alex.kimber\AppData\Local\Microsoft\Windows\INetCache\Content.Word\Spectrum-Fin-between-timber.jpg]

	Entrance doors 
	Profile 22 or IG 
Dark Grey or Black (cira. RAL7016) Composite GRP doors or similar
SBD/Part Q Ironmongary
Cira. RAL 7016
	
	

	Windows & Patio doors
	Dark Grey or Black (cira. RAL7016) uPVC
Profile 22 or Rehau
SBD/Part Q Ironmongary

	
	[image: https://www.profile22.co.uk/wp-content/uploads/2019/08/flush_tilt_turn.jpg]

	Parapet and balcony flashing
& Roof covering
	Axter Edge Flashing or Similar 
Dark Grey (cira. RAL7016)
Axter SinglePly Membrane or Similar (Grey) (roof covering dependant on suppliers designs)
	
	

	rainwater goods
	Axter Black Hopper & uPVC downpipes
	
	[image: https://www.drainagecentral.co.uk/Graphics/Product_Detail_Images/68mm_Round_Downpipe_Hopper_Head_Brett_Martin_BR211Black_Drainage_Central1.jpg]
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