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Introduction
This document is intended to discuss details of the PV array including: Number of panels, peak output and SAP calculation.
PV Array Details
The PV panels selected for this array are JA Solar JAM72S20-450MR.
[bookmark: _GoBack]The total number of panels included in the PV array is 44 Panels, distributed as 36 panels on the flat roof on a 10o pitch and 8 panels on the rear pitch on a 50o pitch. 
All panels are configured in a West facing configuration to building layout and shading of the roof from other buildings in the vicinity.
The annual generation of the array 19,800kWh. The required generation from the SAP calculation was 1,170kWh per flat giving a total of 16,380kWh required across the project.
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