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METHOD  STATEMENT

REPAIRS TO EXISTING GATES

1-2  MARKET PLACE

READING

RG1 2EQ
08 January 2020

	1.0
	SCOPE OF METHOD STATEMENT


	1.1

1.2
	To identify & schedule works in connection with the retention & refurbishment of the existing gates which are part of the Listed Building. 
The works as set out below are to be completed within 1 month of the date of this Method Statement. 



	2.0
	REPAIRS


	2.1
	Remove all existing applied signs, perspex etc & dispose

Fill all fixing holes with two pack epoxy filler & leave ready for decorating

 

	2.2
	Check existing hinges, pivots & bolts are in good condition

Clean & prepare for decorating

Re-grease after decoration & leave in good working order



	2.3
	Take details of existing lettering to curved transom panel

Supply & fix new Letter “C” to replace missing item

New metal letter to be exact type face of existing letters

Prepare all existing & new letters ready for decorating

Sign to read LLOYD’S BANK CHAMBERS


	3.0
	DECORATING


	3.1
	Clean down, sand & lightly apply wire brush to remove any surface rust & prepare ready for painting



	3.2
	Apply primer with rust inhibitor to all surfaces



	3.3
	Repaint all existing Black metal work with 2 No coats of Dulux Metal Shield paint in Black

Pick out “LLOYD’S BANK CHAMBER” lettering & existing transom “SUN RAY” details in Antique 

Gold “Ardenbrite” paint to match existing design



	4.0
	ON COMPLETION OF WORKS


	4.1
5.0

5.1
	On completion of above works, check all moving parts & leave in good working order
ONGOING MAINTENANCE
At all times the sign shall be maintained and kept in good condition.  


	6.0
	APPENDICES


	6.1
	Photographs of existing gates Appendix A


	6.2
	Part plan identifying gates Appendix B



