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1) History, character and significance of the building/site 
2 Paddock Road was built in 1731 and is one of 4 cottages remaining on the street, which were originally cottages for farm workers on Dean Farm. All 4 cottages were Grade II listed in 1976. 
No 4 Has been recently renovated and restored as seen by the previous listed building consent application in 2016. It is semi-detached with No 2. It was extended in 1983 to create a kitchen.
Outside, the main frontage of the original building is built of traditional brick and flint on the lower section. The 1980’s extension is a more modern brick with a pitched tiled roof. Inside, the old cottage is wooden beam construction with beams on show. The 1980’s extension is now a kitchen.
Paddock Road has been extensively developed. There is an industrial estate at the east end of the road and an office building, opposite No 2 and No 4. The cottage furthest down the street (no 8) has been converted to an HMO.
2) Extent and nature of the proposed development 
The proposal is to add a roof light window to the 2nd floor room for fire safety and ventilation. We are looking to fit a conservation approved rooflight window. This would keep in line with the English Heritage and Historic England recommendations.
Currently the access to this room is a narrow wooden staircase. The only window currently in the room is exceedingly small (25cm x 25cm) and is not possible to use as an emergency fire escape. We intend to use this room as a second bedroom but without a safe emergency exit point, we feel it is unsafe to leave a small child sleeping up there.
3) Impact of the development on the heritage asset and justification for the works 
The development would be in keeping with the style of the rest of the building.
The justifications proposed are that:
Currently the access to this room is a narrow wooden staircase. The only window currently in the room is exceedingly small (25cm x 25cm) and is not possible to use as an emergency fire escape. We intend to use this room as a second bedroom but without a safe emergency exit point, we feel it is unsafe to leave a person sleeping up there.

