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Dear

Planning information, 

- Walls - incorrectly repointed and need to be repointed with an appropriate lime mortar
- A better lead flashing needs to be added around the parapet wall/box 
- Windows - repair broken panes of glass, prepare and redecorate and ease and adjust in the next few years. 
- Repair or replace dated electrics
- Replace boiler and central heating system (inc radiators)
- To add an inter-linked fire alarm system 
[bookmark: _GoBack]- Lastly, I discussed potentially opening up the utility room ceiling to full height - the surveyor said this would help with condensation issues we may get in this area if used for washing clothing etc.
----------------------------------------------------------------------------------------------------------------------------
The following list which I have expanded on for clarity:

1) Walls- incorrectly repointed and need to be repointed with an appropriate lime mortar. Previously this has received retrospective planning permission however at some point it is likely the work will need to be repeated with the correct mortar as it is not allowing the property to breathe.

2) Roof repairs:
- A better lead flashing needs to be added around the parapet wall/box gutter area where the hopper head is overflowing, and our buildings surveyor recommends the downpipe is discharged away from the building. 
- Slipped slates need to be fixed

3) Windows- repair broken panes of glass, prepare, redecorate, ease and adjust. 

4) Kitchen and Utility refit (plans available) Including opening up the utility room ceiling to full (sloped) height - the surveyor said this would help with condensation issues we may get in this area if used for washing clothing etc.

5) Repair or replace dated electrics including adding a new fuse board and replacing dated socket points

6) Replace boiler and central heating system in favour of a combination boiler. Boiler to relocate into upstairs airing cupboard and (much smaller than current) flue to exit out of internal facing rear side wall. Radiators to be replaced over time with traditional style radiators. 

7) Addition of an inter-linked fire alarm system

8) Installation of burglar alarm

9) Instillation of electric garage door(s) - opening inwards and keeping the same current facade

10) Restoration of ceiling rose in living room, dining room and hallway - they have been painted many times and the thick layers of paint have reduced the visibility of the carved detail

11) 50%-75% paving stones removed from garden to enable turf lawn to be laid.

12) Refit top floor bathroom 3-piece suite including replacement metal window frame in favour of draft free velux window.

Regards,
Martin Stuart.






















Regards,



Martin Stuart
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