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INC Design Associates Ltd

1 Dudley Court North, Waterfront East

Level Street

Brierley Hill

DY5 1XP
	             Frances Martin

             Executive Director for Economic Growth 

             and Neighbourhood Services

Civic Offices, Bridge Street,

Reading, RG1 2LU

 0118 9373787

Our Ref: 190937
Your Ref: PP-07928640
Direct : 0118 9372023
e-mail: susanna.bedford@reading.gov.uk










        Date: 20th September 2019 

	Your contact is:
	Susanna Bedford, Planning 


Dear INC Design Associates Ltd,

TOWN AND COUNTRY PLANNING ACT 1990

Application Reference: 190937

Application type: Approval of Conditions





Address: Land at Corner of Addison Road and Meadow Road Reading  
Proposal: Application for approval of details reserved by condition 13 (Validation Report) of application 130882.  

I refer to your application as described above. 

Condition 13 requires: The remediation scheme shall be implemented in accordance with the

approved timetable of works. A validation report (that demonstrates the effectiveness of the remediation carried out) shall be submitted to and approved by the Local Planning Authority prior to construction of the development.

Reason. To ensure appropriate control and remediation of land contamination, in accordance with Policy CS34 of the Reading Borough LDF Core Strategy 2008 (altered 2015).
Information has been submitted in order to discharge this condition in relation to 

i) ground water (also reviewed by the Environment Agency) and,  

ii) soil testing  
Information submitted: 12th June 2019 
· ‘Validation Report Following Remedation on a site at the Corner of Meadow Road and Addison Road, Caversham, Reading’ Dated 21st May 2019 Ref G/031850/005 produced by KF Geotechnical 

· Soil sample analysis pack of documents produced by ‘pmc Soil Solutions’ (individual dates on each sample)
Further reference was sought by the Environment Agency to include Total Petroleum Hydrocarbons in the validation sampling for this site.

Information submitted: 23rd August 2019 (via email) 
ChemTest Report (to include TPH) ref Standard Report 19-25854-1 dated 6th August 2019 produced by KF Geotechnical 
CC
The Environment Agency reviewed these soil validation test results for Plots 1 to 5 and from a groundwater quality perspective were able to recommend the discharge of condition 13. 
Additional clarification was required by Reading Borough Council officers; and further information submitted: 

Information submitted: 19th August 2019 Email from T.Voller containing Details of the Vapour Barrier installed on drawing No EO119-001 rev D (produced by INC Architects dated 16.1.2019); and confirmation that no gas protection measures need to be incorporated (as specified within the GES Contamination Assessment dated December 2018 p28-29 attached within this email) 

Information submitted: 6th September 2019 Email from Craig Lewarne, Building Control Officer to confirm the proposed and approved single size stone aggregate was installed to create a hydraulic break to 150mm depth between layers of geotextile membranes in all areas identified on KF Geotechnical report.
Information submitted: 12th September 2019 
REVISED ‘Validation Report Following Remedation on a site at the Corner of Meadow Road and Addison Road, Caversham, Reading’ Dated 12th September Ref G/031850/005R produced by KF Geotechnical
Therefore based on the information submitted via email, listed above, and the updated Validation Report dated 12th September Ref G/031850/005R,  Condition 13 can be discharged.

Please note that it is the responsibility of the developer to ensure that all relevant conditions are complied with during the construction and/or subsequent use of the development.

Should you wish to discuss this matter further, please contact me by email or the direct line as above.

Yours sincerely

Susanna Bedford 

Susanna Bedford

Principal Planning Officer
www.reading.gov.uk 
Text 81722
DX 40124 Reading (Castle Street)

