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FILE NOTE

PROJECT NO.:		1976			
PROJECT NAME:	153 HEMDEAN ROAD, READING, RG4 7QU 
[bookmark: _GoBack]SUBJECT:		Planning Condition Material Schedule Rev C
DATE:			07 October 2019 
AUTHOR:		MC
ACG REF:		1976_401_191007_Material Schedule C

	No.
	Type
	Specification
	Material Sample Photographs
	Material Sample Precedent
	Location/Type

	01
	Brickwork
	Supplier: Bespoke Brick Company
Product Type: Brick
Product Reference/Finish: Cinder Coal White
Mortar Colour: White 
	
[image: /Volumes/0_Projects/239_Buckhold Road_Wandsworth/239_Production/239_Images & Models/Material Sample Photos/Alucobond Midnight Copper 920_3D_p edit.jpg]

	
	External Walls

	02
	Render
	Supplier: Sto Ltd
Product Type: StoTherm Classsic
Product Reference/Finish: White


	
[image: ]

	
	External Walls

	03
	Slate Roofing
	Supplier: Marley Eternit
Product Type: Roofing Slates
Format: 600mm (H) x 300mm (W)
Product Reference/Finish: Thrutone Fibre Cement Slates – Blue/Black
	
[image: /Users/matthewchamberlain/Downloads/Garsdale-product-page-2.jpg]
	
[image: /Users/matthewchamberlain/Downloads/Garsdale-2017-Product-Page.jpg]

	Roofs

	04
	Windows
	Supplier: IdealCombi
Product Type: Futura+ 53mm inward opening range for tilt and turn. Fixed Panes same range
Composite Windows
Product Reference/Finish: Anodised HAI Horsens B1
	
[image: /Volumes/0_Projects/239_Buckhold Road_Wandsworth/239_Production/239_Images & Models/Material Sample Photos/RAL 7038.png]

	
[image: ]

	External Windows 

	05
	Sliding Doors
	Supplier: Keller
Product Type: Minimal Windows
Thermally Broken Aluminium Windows
Product Reference/Finish: Anodised HAI Horsens B1
	
[image: /Users/matthewchamberlain/Desktop/Screen Shot 2018-07-15 at 06.32.18.png]
	
[image: /Users/matthewchamberlain/Downloads/KELLER_Brussels-Residence-minimal-windows_3590.jpg]
	External Walls – to Balcony Areas

	06
	Chain Link Fencing
	Chain Link PVC Coated (green) galvanised core

https://www.jacksons-fencing.co.uk/fencing/roll/chain-link-family-pvc
	Proprietary
	Proprietary
	Boundary fences to reinforce existing hedging, set 150mm above prevailing ground levels
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