


Emails from applicant with further details – 171539/LBC

From: John Burnett 
Sent: 22 September 2017 09:21
To: Amoah, Alison
Subject: Re: 35 Coley Hill - 171538/FUL & 171539/LBC

Alison

I had a meeting with my electrician and he said that he could upgrade the smoke alarms which were installed when tReading Council owned the property as a refuge.  They are ceiling mounted wired smoke and CO2 detectors which are radio linked.  This seems to be the perfect solution as it will not require any channeling of the walls etc…  

Do you require the size and make of the detectors?

From: John Burnett 
Sent: 19 December 2017 11:30
To: Amoah, Alison
Subject: Re: 35 Coley Hill - 171539/LBC
This is an EXTERNAL EMAIL. STOP. THINK before you CLICK links or OPEN attachments.
Dear Alison

Apologies for the delay in getting back to you.  

I have made another site visit and checked the ceilings which have all been replaced by the Council when it was in their ownership.  They seem to be hour fire resistant with expanded metal structure.  The ceiling roses are also not even plaster and clearly relatively new.  The location of the smoke alarms will be on the flat part of the ceiling  and will not interfere with the ceiling roses.  They can not be located on the walls as they will not function properly there.  Further this will require ugly surface wiring to provide power.  This is not necessary when located on the ceiling as the power will come from the central light pendant and will be   in the floor void above.  This is the method used by the Council when they fitted their smoke alarms on site.

As the alarms are all radio linked they require no channeling.  The main fire alarm board will be located by the front door where there is already power which I presume was put in by the Council when they would have had an alarm in the building.  The electrician said that the smoke alarms will be the standard size and no different from the ones installed by the Council which are still on site.  The location of all the fire equipment is marked on the plan originally submitted as part of the application.

I do not believe that the installation will be any more intrusive than erecting a picture and may not actually need permission.


From: John Burnett 
Sent: 08 September 2018 04:27
To: Amoah, Alison
Subject: Re: 35 Coley Hill - 171539/LBC
This is an EXTERNAL EMAIL. STOP. THINK before you CLICK links or OPEN attachments.
Dear Alison

I have enclosed pictures of the Smoke detectors and a specification including dimensions.

The Four existing  smoke alarms will be replaced with new in the same locations.  The rest will be fixed on the smooth section of the ceiling away from the coving and center rose.  There will not be a control box in the hall.

The smoke alarms will be screwed to the ceiling and attached to the existing mains cable feeding the light fitting.  The ceilings are not original lath and plaster as they were replaced by Reading Council during their ownership of the property.

[bookmark: _GoBack][image: cid:32226D86-5AC2-4D8A-80FE-981D7345C2A0][image: cid:6611EC2E-7BFD-400E-9F55-42479230F794]









image1.png
SPECIFICATION
Alarm Product Type
Alarm Sensor Type
Battery Duration
Battery Type

Brand

CE Standard (Tested to EN...)
Fixings Supplied
Manufacturer Guarantee
Model Name

Model No

Pack Size

Pleces in Pack/Case
Power Source

Power Voltage Supply
Product Depth

Product Diameter
Product Type

Total Product Weight

Wireless/Wired

230V. EN 14604: 2005.

‘Smoke Alarms.
Optical
10-Year Sealed Battery (Lithium)
Lithium
FireAngel Pro
EN 14604: 2005.
Fixings Supplied
2 Year Manufacturer's Guarantee (T&Cs Apply)
Wireless Interlink Thermoptek
WST-230
1
1
Mains & Battery-Powered
230V
s2mm
141 mm
Wireless Interlink Thermoptek Smoke Alarm
0284 kg

Wireless.
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