


Delegated Application Report 				          Target Date: 07/08/17
Address: 8 Shenstone Road
Application No: 170921/CLP
Proposal: Loft conversion with rear box dormer and removal of chimney
Case Officer: Tom Hughes
Introduction and Proposal
The application site is a two storey semi-detached property with a pitched roof. Chimneys protrude from the forward and rearward roof slopes. A two storey gable projects to the rear. A lean-to adjoins the side elevation. The surrounding area is predominantly residential, comprised of properties of various styles and design. 
The proposal is for a loft conversion and the provision of a rear box dormer. The chimney located to the rearward roof slope would be removed to facilitate the proposal. The box dormer would project to a depth of 4.2, extending at a width of 4.2m. The box dormer would have a maximum height of 2.6m. The box dormer would be set back from the existing eaves by 0.3m, and set down from the ridgeline of the existing roof by 0.3m. The box dormer would have a total volume of 22.93 cubic metres. The face and cheeks of the dormer would be clad in tiles to match the existing property. Two windows would be located to the rearward elevation.
Plans Submitted
The agent supplied the following, received on 6th June 2017:
Drawing No: 03 – Existing Floor Plans, Roof Plan and Elevations
Drawing No: 04 – Proposed Floor Plans, Roof Plan and Elevations
Subsequently, the agent supplied the following, received on 7th June 2017:
Drawing No: 1 – Site Location
Drawing No: 2 – Block Plan
Relevant Planning History
170583/CLP – Loft conversion and rear box dormer – Permitted 08/05/17
Summary of Consultations
No consultations were undertaken as it is not required for an application of this type.
Relevant Planning Policy and Guidance
National Planning Practice Guidance
The Town and Country Planning (General Permitted Development) (England) Order 2015 (GPDO)
Permitted development rights for householders – Technical Guidance April 2017
Assessment
A Certificate of Lawfulness for a proposed development has been submitted as the applicant considers the proposal falls within the permitted development rights of the property. 
The proposed loft conversion with rear box dormer and removal of chimney must be assessed to ensure that it complies with the conditions of Class B and Class G, Part 1, Schedule 2 of the Town and Country Planning (General Permitted Development) (England) Order 2015, which relate to ‘additions etc to the roof of a dwellinghouse’ and ‘chimneys, flues etc on a dwellinghouse’.
The relevant conditions of the GPDO for a loft conversion with a rear box dormer and removal of chimney, which is not listed or in a conservation area, are as follows: 
B.1 Development is not permitted by Class B if:
B.1 (a) permission to use the dwellinghouse as a dwellinghouse has been granted only by virtue of Class M, N, P or Q of Part 3 of this Schedule (changes of use); complies
B.1 (b) any part of the dwellinghouse would, as a result of the works, exceed the height of the highest part of the existing roof; complies
B.1 (c) any part of the dwellinghouse would, as a result of the works, extend beyond the plane of any existing roof slope which forms the principal elevation of the dwellinghouse and fronts a highway; complies
B.1 (d) the cubic content of the resulting roof space would exceed the cubic content of the original roof space by more than (i) 40 cubic metres in the case of a terrace house, n/a or (ii) 50 cubic metres in any other case; complies, the cubic content of the resulting roof space would exceed the cubic content of the original roof space by 22.93 cubic metres
B.1 (e) it would consist of or include (i) the construction or provision of a veranda, balcony or raised platform, complies or (ii) the installation, alteration or replacement of a chimney, flue or soil and vent pipe; complies, subject to Class G or
B.1 (f) the dwellinghouse is on article 2(3) land. complies
Conditions
B.2 Development is permitted by Class B subject to the following conditions:
B.2 (a) the materials used in any exterior work must be of a similar appearance to those used in the construction of the exterior of the existing dwellinghouse; complies
B.2 (b) the enlargement must be constructed so that (i) other than in the case of a hip-to-gable enlargement or an enlargement which joins the original roof to the roof of a rear or side extension (aa) the eaves of the original roof are maintained or reinstated; complies and (bb) the edge of the enlargement closest to the eaves of the original roof is, so far as practicable, not less than 0.2 metres from the eaves, measured along the roof slope from the outside edge of the eaves; complies and (ii) other than in the case of an enlargement which joins the original roof to the roof of a rear or side extension, no part of the enlargement extends beyond the outside face of any external wall of the original dwellinghouse; complies and 
B.2 (c) any window inserted on a wall or roof slope forming a side elevation of the dwellinghouse must be (i) obscure-glazed, complies and (ii) non-opening unless the parts of the window which can be opened are more than 1.7 metres above the floor of the room in which the window is installed. complies
Interpretation of Class B
B.3 For the purposes of Class B, “resulting roof space” means the roof space as enlarged, taking into account any enlargement to the original roof space, whether permitted by this Class or not.
B.4 For the purposes of paragraph B.2(b)(ii), roof tiles, guttering, fascias, barge boards, and other minor roof details overhanging the external wall of the original dwellinghouse are not to be considered part of the enlargement.
G.1 Development is not permitted by Class G if:
G.1 (a) permission to use the dwellinghouse as a dwellinghouse has been granted only by virtue of Class M, N, P, or Q of Part 3 of this Schedule (changes of use); complies
G.1 (b) the height of the chimney, flue or soil and vent pipe would exceed the highest part of the roof by 1 metre or more; complies or
G.1 (c) in the case of a dwellinghouse on article 2(3) land, the chimney, flue or soil and vent pipe would be installed on a wall or roof slope which (i) fronts a highway, complies and (ii) forms either the principal elevation or a side elevation of the dwellinghouse. complies
Recommendation
Sufficient evidence has been provided to demonstrate that a Certificate of Lawfulness should be granted for the proposed loft conversion with rear box dormer and removal of chimney. 
The proposal has been assessed against the Town and Country Planning Act 1990 (as amended) and Class B and Class G, Part 1, Schedule 2 of the Town and Country Planning (General Permitted Development) (England) Order 2015. It can be confirmed that the proposed operation would be lawful for planning purposes on the basis of the following drawings: 
Drawing No: 04 – Proposed Floor Plans, Roof Plan and Elevations (received 6th June 2017)
Drawing No: 02 – Block Plan (received 7th June 2017)
Therefore the Local Planning Authority can issue the applicant with a Certificate of Lawfulness for the proposed development.
Informatives
Building Regulations
Encroachment and Party Wall Act
Construction and Demolition
Materials
Bats
[bookmark: _GoBack][image: ]




image1.png
il
— 9 e ’
o 4 < 0y w mm_,m
w 0@0 wmw%%o @‘ Wﬁ
3 H ) > %s »%bm m
el O & Sl
3 @ 5 g0 > 8 M«% H
LW %Bfﬂ, @ \\\\ a 7 m
AT @ h%%ﬂwwy %@ §
ALY N %@% MV\ s |
(L] §® ‘\\\\ @@%W 0§ .
J NG - .
5 &S S




