


Delegated Application Report 				          Target Date: 14/09/17
Address: 29 Carnarvon Road
Application No: 171216/CLP
Proposal: Refurbishment of basement and light well
Case Officer: Tom Hughes
Introduction and Proposal
The application site is a semi-detached property with a hipped roof. The property benefits from a basement, with a light well to the northward side elevation. The surrounding area is predominantly residential.  
The proposal is for the refurbishment of the basement and the existing light well, to provide a secondary escape. The existing light well would be replaced by a glazed canopy with metal supports. The canopy would have a maximum height of 1m above ground level. The canopy would extend at a width of 0.8m and project to a depth of 1.6m. Materials have been selected to match those of the existing property.  
Plans Submitted
The agent supplied the following, received on 20th July 2017:
Site Location
Drawing No: IS 2017/01 – Block Plan, Existing Floor Plans, Elevations and Sections
Drawing No: IS 2017/02 – Proposed Floor Plans, Elevations and Sections
Relevant Planning History
None. 
Summary of Consultations
No consultations were undertaken as it is not required for an application of this type.
Relevant Planning Policy and Guidance
National Planning Practice Guidance
The Town and Country Planning (General Permitted Development) (England) Order 2015 (GPDO)
Permitted development rights for householders – Technical Guidance April 2017
Assessment
A Certificate of Lawfulness for a proposed development has been submitted as the applicant considers the proposal falls within the permitted development rights of the property. 
The proposed refurbishment of basement and light well must be assessed to ensure that it complies with the conditions of Class A, Part 1, Schedule 2 of the Town and Country Planning (General Permitted Development) (England) Order 2015, which relates to the ‘enlargement, improvement or other alteration of a dwellinghouse’.
The relevant conditions of the GPDO for a refurbishment of basement and light well, which is not listed or in a conservation area, are as follows: 
A.1 Development is not permitted by Class A if:  
A.1 (a) permission to use the dwellinghouse as a dwellinghouse has been granted only by virtue of Class M, N, P or Q of Part 3 of this Schedule (changes of use); complies
A.1 (b) as a result of the works, the total area of ground covered by buildings within the curtilage of the dwellinghouse (other than the original dwellinghouse) would exceed 50% of the total area of the curtilage (excluding the ground area of the original dwellinghouse); complies
A.1 (c) the height of the part of the dwellinghouse enlarged, improved or altered would exceed the height of the highest part of the roof of the existing dwellinghouse; complies
A.1 (d) the height of the eaves of the part of the dwellinghouse enlarged, improved or altered would exceed the height of the eaves of the existing dwellinghouse; complies
A.1 (e) the enlarged part of the dwellinghouse would extend beyond a wall which (i) forms the principle elevation of the original dwellinghouse; complies or (ii) fronts a highway and forms a side elevation of the original dwellinghouse; complies
A.1 (f) subject to paragraph (g), the enlarged part of the dwellinghouse would have a single storey and – (i) extend beyond the rear wall of the original dwellinghouse by more than 4 metres in the case of a detached dwellinghouse, or 3 metres in the case of any other dwellinghouse, complies or (ii) exceed 4 metres in height; complies
A.1 (g) until 30th May 2019, for a dwellinghouse not on article 2(3) land nor on a site of special scientific interest, the enlarged part of the dwellinghouse would have a single storey and – (i) extend beyond the rear wall of the original dwellinghouse by more than 8 metres in the case of a detached dwellinghouse, or 6 metres in the case of any other dwellinghouse, complies or (ii) exceed 4 metres in height; complies
A.1 (h) the enlarged part of the dwellinghouse would have more than a single storey and – (i) extend beyond the rear wall of the original dwellinghouse by more than 3 metres, complies or (ii) be within 7 metres of any boundary of the curtilage of the dwellinghouse opposite the rear wall of the dwellinghouse; complies
A.1 (i) the enlarged part of the dwellinghouse would be within 2 metres of the boundary of the curtilage of the dwellinghouse, and the height of the eaves of the enlarged part would exceed 3 metres; complies
A.1 (j) the enlarged part of the dwellinghouse would extend beyond a wall forming a side elevation of the original dwellinghouse, and would – (i) exceed 4 metres in height, complies (ii) have more than a single storey, complies or (iii) have a width greater than half the width of the original dwellinghouse; complies
A.1 (ja) any total enlargement (being the enlarged part together with any existing enlargement of the original dwellinghouse to which it will be joined) exceeds or would exceed the limits set out in sub-paragraphs (e) to (j); complies
A.1 (k) it would consist of or include – (i) the construction or provision of a verandah, balcony or raised platform, complies (ii) the installation, alteration or replacement of a microwave antenna, complies (iii) the installation, alteration or replacement of a chimney, flue or soil and vent pipe, complies or (iv) an alteration to any part of the roof of the dwellinghouse. complies
A.2 In the case of a dwellinghouse on article 2(3) land, development is not permitted by Class A if:
A.2 (a) it would consist of or include the cladding of any part of the exterior of the dwellinghouse with stone, artificial stone, pebble dash, render, timber, plastic or tiles; n/a
A.2 (b) the enlarged part of the dwellinghouse would extend beyond a wall forming a side elevation of the original dwellinghouse; n/a
A.2 (c) the enlarged part of the dwellinghouse would have more than a single storey and extend beyond the rear wall of the original dwellinghouse; n/a
A.2 (d) any total enlargement (being the enlarged part together with any existing enlargement of the original dwellinghouse to which it will be joined) exceeds or would exceed the limits set out in sub-paragraphs (b) and (c).
Conditions
Development is permitted by Class A subject to the following conditions:
A.3 (a) the materials used in any exterior work (other than materials used in the construction of a conservatory) must be of a similar appearance to those used in the construction of the exterior of the dwellinghouse; complies
A.3 (b) any upper-floor window located in a wall or roof slope forming a side elevation of the dwellinghouse must be (i) obscure-glazed, complies and (ii) non-opening unless the parts of the window which can be opened are more than 1.7 metres above the floor of the room in which the window is installed; complies and
A.3 (c) where the enlarged part of the dwellinghouse has more than a single storey, or forms an upper storey on an existing enlargement of the original dwellinghouse, the roof pitch of the enlarged part must, so far as practicable, be the same as the roof pitch of the original dwellinghouse. complies
Recommendation
Sufficient evidence has been provided to demonstrate that a Certificate of Lawfulness should be granted for the proposed refurbishment of basement and light well.
The proposal has been assessed against the Town and Country Planning Act 1990 (as amended) and Class A, Part 1, Schedule 2 of the Town and Country Planning (General Permitted Development) (England) Order 2015. It can be confirmed that the proposed operation would be lawful for planning purposes on the basis of the drawings received on 20th July 2017:
Drawing No: IS 2017/02 – Proposed Floor Plans, Elevations and Sections
Therefore the Local Planning Authority can issue the applicant with a Certificate of Lawfulness for the proposed development.
Informatives
Building Regulations
Encroachment and Party Wall Act
Construction and Demolition
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