Discharge of Conditions  St Peters avenue RG4 7DP 
Application No. 150172

3.
a)  Materials for external surfaces
Unit 1 
Roof. Spanish slate as per picture  600 x 400 pic 1 











Ground floor , off  white resin render ( pic 2 ) 


First floor , Natural Siberian lartch 120 x 19 mm tongue and groove pic 4 




Unit 2
Roof. Spanish slate as per picture  600 x 400 







Ground Floor , brick Hardwicke Minster Beckstone Mixture 65mm pic 3 
Pic 2

First floor. Off white resin render  pic 2
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