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Internal Memorandum

	

	To:  
	Anthony Scholes
	Your Ref:
	PL/24/1055

	From:
	Rebecca Moon - Environmental Health Officer
	My Ref:
	EP /780295

	Date consultation received: 23/08/2024
	Date: 19 September 2024

	


Application Number: PL/24/1055  
Premises Address:  185a Oxford Road Reading  RG1 7UZ
Application For: Proposed upward extension to provide 1 studio flat  

Environmental Protection concerns

· Noise impact on development

· Construction and Demolition phase

Noise impact on development

The location is exposed to noise from the busy Oxford Road and surrounding commercial uses including plant noise to the rear.

A noise assessment should be submitted in support of applications for new residential proposed in noisy areas.

The noise assessment will be assessed against the recommendations for internal noise levels within dwellings and external noise levels within gardens / balconies in accordance with BS 8233:2014 and WHO guidelines for Community Noise. The report should identify any mitigation measures that are necessary to ensure that the recommended standard is met. 

The noise assessment data should also include noise events (LAMax) and the design should aim to prevent noise levels from noise events exceeding 45dB within bedrooms at night, as this is linked with sleep disturbance.

Internal noise criteria (taken from BS8233:2014)

	Room
	Design criteria 
	Upper limit

	Bedrooms (23:00 to 07:00)
	<30dB LAeq,8hour
	

	Living rooms (07:00 – 23:00)
	<35dB LAeq,16hour
	

	Gardens & Balconies
	<50dB LAeq,T
	<55dB LAeq,T


Where the new residential use may be affected by noise from commercial premises, the assessment should also include consideration of the impact of the commercial noise sources either by using BS4142:2014 A 2019 methodology, by applying additional penalties to the BS8233 guideline noise levels and/or other relevant guidance for particular noise sources such as music noise, as penalties may need to be applied to the acceptable internal noise levels to take into account non anonymous noise sources. 
If the noise assessment cannot be provided prior to a decision, I recommend a condition is attached to any consent requiring a noise assessment to be submitted prior to commencement of development and any approved mitigation measures implemented prior to occupation to show that recommended noise levels in the table above can be met.

The noise assessment will need to identify the external noise levels impacting on the proposed site. 

Noise mitigation is likely to focus on the weak point in the structure; glazing. Given that the acoustic integrity would be compromised should the windows be opened, ventilation details must also be provided, where mitigation relies on closed windows. Ventilation measures should be selected which do not allow unacceptable noise ingress and should provide sufficient ventilation to avoid the need to open windows in hot weather, however non-openable windows are not considered an acceptable solution due to the impact on living standards.

I recommend the following condition.

· N9
NOISE ASSESSMENT & MITIGATION RESIDENTIAL (TO BE SUBMITTED)

No development shall commence on site until a detailed scheme, informed by an assessment of the current noise environment, for protecting the dwellings from the external noise environment of the area has been submitted to and approved, in writing, by the Local Planning Authority.  The scheme itself shall be designed, specified and constructed so that the sound insulation performance of the structure and the layout of the dwellings are such that the indoor ambient noise levels do not exceed the values detailed in Table 4 of BS 8233:2014 and the and that the individual noise events do not exceed 45 dB LA,max,F more than 10 times a night.  Appropriate penalties shall be applied for non-anonymous noise sources.  Where opening windows will lead to an internal noise level increase of 5 dBA or greater above BS 8233:2014 recommended internal levels, the scheme shall include provision of alternative mechanical ventilation with minimum performance equivalent to a mechanical heat recovery (MVHR) system with cool air bypass as an alternative means of cooling and ventilation.  Noise from the system should not result in BS8233 internal levels being exceeded.

Thereafter, the development shall not be carried out other than in accordance with the approved scheme which shall be completed before any part of the accommodation hereby approved is occupied, unless the Local Planning Authority otherwise agrees in writing.

REASON: These details are required due to insufficient information being contained within this submission and in order to safeguard the amenity of occupants in accordance with Policy CC8 of the Reading Borough Local Plan 2019.
Construction and demolition phases – informative
We commonly receive complaints about noise and dust caused by construction and demolition works, particularly working outside reasonable hours and about smoke from bonfires associated with the burning of waste on site of minor developments.

I recommend the following informative is attached to help prevent complaints.

Recommended Informative

Noisy construction, demolition and associated activities should be restricted to between the hours of 08:00hrs to 18:00hrs Mondays to Fridays, and 08:00hrs to 13:00hrs on Saturdays, with no noisy works taking place at any time on Sundays and Bank or Statutory Holidays.

There should be no burning of waste on the site.

Dust emissions to air should be minimised by good practice measures. 

Capping of redundant drains/sewers should be carried out to reduce the risk of vermin ingress.
If you have any queries please contact me.

Kind regards,

Rebecca Moon - Environmental Health Officer
