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                                     Method Statement in relation to construction of Twin Wire
                                     Mesh Security fencing with additional measures for protection
                                     of trees
                                              
                
                                              
                       

    1.  Objective To construct a 230-metre security fence of Twin Wire Mesh around car
                          parking area.  The fence will be 2.4 metres in height 

    2.  Address of project.  Atlantic House, Imperial Way, Reading RG2 0TD
  
    
    3. Special Measures to protect trees.  On the northern boundary of the car park (on 
         adjacent property) there are a number of mature trees.  17 Alder (Alnus 
         glutinosa) 2 Goat Willow (Salix caprea) and Silver Birch (Betula Pendula)  This 
         area measures 83.5 metres.  The fence will cover the boundary.  To 
         ensure the fence does not interfere with the trees and vice versa it will be 
         necessary to lift the crowns of the trees on the new fence side by 2.6 metres
         reducing the lateral branches to this point by one metre.  This will leave ample room
         for construction of the fence and due to the vigorous nature of the trees will not
         impact them visually.  NB There is one Alder which is of poor vigour and should be
         removed.  Hand tools should be used with the removal of the branches.

      4. Machinery to be used (tree work).  Silky hand saws, Oil and Steel MEWP, Forst
           chipper.

      5. Personnel (tree work) Four staff members will be used for this project.  All staff to
         have correct PPE

      6. Date of works TBA

      7.  Loler and RIDOR.  All recommendations have been met.

8.  All work to be completed to BS3998.  British Standard tree work recommendations
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