Good morning,

Thank you for sending this across.

As per the Council’s waste management guide, bin storage areas must comply with the following:
1. All bins must be fully accessible from the front face, to allow for easy depositing
of waste. 
1. Layouts that require bins to be swapped round mid-week are permissible if it is
demonstrated that there will be on-site management presence at the
development. 
1. There must be a minimum of 150mm clearance around and between each bin within a
storage area. 
1. Where there is more than one bin within a storage area, there must be 2m clearance in
front of each bin to enable it to be accessed and safely moved without needing
to move any of the other containers.
1. All doors and alleys must be at least 2m wide to allow for safe manoeuvring of
bins.
1. The minimum internal height for a bin storage area and any access doorways is
2m. 
1. To allow the lids to be opened fully, there should be no other internal fixtures
or fittings that reduce the clearance above the bins. 

Based on the plans shown, I expect that the doors to the bin store would not be wide enough for safe manoeuvring of bins. Please also note that for crews to retrieve bins from the bin store there would need to be an external door directly into the bin store itself.  Bins cannot be left on the pavement at any time in this location so it would not be suitable for bins to be presented for collection.

The Council’s standard household waste collection service is for a fortnightly general waste collection, fortnightly recycling collection and weekly food waste collection. Glass recycling collections are being introduced in the near future and the glass bins will be collected fortnightly.
A development containing 4 residential units with communal facilities would need to have space for the below bins:
1. 2 x 240L general waste bins
1. 3 x 360L recycling bins
1. 1 x 240L food waste bin
1. 1 x 240L glass bin

The bin store on the plan is not big enough to house the required number of bins, whilst remaining compliant with the above bin store requirements.

