	
	RBC Comment
	Packaged Living response
	Comments

	1
	ATE Assessment - Updated to account for routes to Public Transport and Local Amenities
	Updated information to be provided to RBC Transport for comment
	Stantec have agreed with RBC that the ATE Tool is not required and that the previous Tech Note can be updated to include all facilities, not focus on Education. This will be issued to RBC via separate issue.

	2
	Cycle Parking Spaces and seating cubes within public highway (Tow-path) - Need to be relocated to count towards visitor parking
	Cycle Parking spaces have been removed from the towpath.  Relocation options are now provided for RBC Transport and Planning’s consideration.
	Extract below identifies relocation of spaces to the public courtyard. 

[image: ]

	3
	Pedestrian route north of the bin presentation area needs to be 2m, currently there are conflicts with the landscaped area
	See updated drawing 0006_P11
Extract inserted to show path provision
	[image: ]

	4
	Bin presentation area is considered not to work in practice. There are potential conflicts with pedestrians and vehicles
	See updated drawing 0006_P11
Extract of Plan inserted
Extract of Landscape inserted 
	Plan shows that refuse area will be denoted by metal studs
[image: ][image: ]

	5
	Refuse strategy - Agreement with the RBC Waste team to ensure drawings are illustrating the correct number of bins
	13no 1,100l Eurobins and 13no 240l are shown. See updated drawing 0006_P11
	For the purpose of planning we believe that we have shown sufficient evidence to support the application, however if RBC seek a formal Waste Strategy agreement this can be conditioned.

	6
	Vastern Road Trees - Interaction between trees, signs and Clearwater Court
Western tree position has been moved and reduces the effective cycleway width, this needs to be relocated to its original position
	Further to input from Hexa, 3no trees are proposed to the front of the building, which accounts for the 2no trees previously proposed on Vastern Road and relocation of the tree previously located on the south-western corner of the building. See updated drawing A4012E-ASA-XX-00-DR-L-0200, Rev P5
	Visibility issues no longer relevant to trees given relocation within the red line and to the front of the building.

	7
	Norman Place – location that visibility is taken from needs updating
	
	Not Required following Tree Removal

	8
	Vastern Road – dimensions and location that visibility is taken from needs updating 
	
	Not Required following Tree Removal 

	9
	Car Park Access – Corduroy paving/Visibility Splay to the North / Give Way markings, needs updating
	See updated drawing 0023A_P05
	Landscape plan also updated to remove tactile paving.

	10
	Loading Area – southern drop kerb to be extended
	See updated drawing 0023A_P05
	Extended Drop Kerbs Provided 

	11
	Cycle parking to front of building – to be updated in line with standards
	See updating drawing A4012E-ASA-XX-00-DR-L-0200, Rev P5
	Amendments as per RBC Standards included 

	12
	Pumping Appliance Tracking – illustrate the distance between the vehicle and building is greater than 500mm
	See updated drawing 0021_P09 
	Minor encroachment inside clearance areas, but these are minimal and plans shows sufficient safe width to support fire access to rear of building 
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