FLOOR RISK ASSESSMENT

The application proposal is for a single storey rear extension at; 
89 Gosbrook Road Caversham Berks RG4 8BU 
The ground floor level within the proposed development will be set no lower than the existing level. 

This will ensure that the existing property, including the extension, will not have an increased risk of flooding. 

As further precaution the new building work will follow the guidelines in the document;
Improving the flood performance of new buildings

www.planningportal.gov.uk/uploads/br/flood_performance.pdf
The extension is 21 sqm

All precautions will be considered and a resilient design will be incorporated in the construction to allow for the drainage and clearance of flood water should such an event occur.

Drainage, soakaways, foundation and ground floor will be as appropriate for a flood plain area. The new floor slab will be constructed with no sub floor voids

and water resistant cavity fill and internal plaster will be used.
The proposed extension is not lower than the existing floor level of the house and will include the measures referred to above. The proposed development is therefore not considered to have an adverse effect on a watercourse, floodplain or its flood defences, as demonstrated by the numerous similar developments that have been permitted in the locality in the past.

