Proposed Rooflight Schedule
Site: 92 Audley Street, Reading RG30 1BS
Proposal: Installation of three conservation-style flush rooflights within the existing roof slopes.
	Reference
	Product
	Size
	Qty

	RL1
	VELUX GGL CK02 2570H Conservation Centre-Pivot Roof Window
	550 x 780 mm
	1

	RL2
	VELUX GGL CK02 2570H Conservation Centre-Pivot Roof Window
	550 x 780 mm
	1

	RL3
	VELUX GGL MK08 2570H Conservation Centre-Pivot Roof Window
	780 x 1400 mm
	1


General Specification
· All rooflights to be conservation-style centre-pivot roof windows.
· Rooflights to be installed flush within the existing roof plane in accordance with the manufacturer’s installation instructions.
· Existing roof profile, pitch and ridge height to remain unchanged.
· No dormers, raised roof structures or alterations to the roof form are proposed.
· External finish to match the manufacturer’s conservation specification (or approved equivalent).
· Manufacturer’s product literature accompanies this application.
